Here’s a summary of our action items:
 
1. Chad: electrical schematic/diagram for high speed camera to larger vehicles (change of camera from high-speed to high-sensitivity in design; get model information from Alana; in progress)
2. Kakani: analyze data!!! (completed)
3. Alana: test video output on HDMI (completed; A7S works, not sure about when firmware for A7Sii will be updated)
4. Dale: purchase fiber penetrator, at least 6 m in length (narrowing down; going with 8 m long penetrator with 0.5 m pigtails; completed; waiting to hear back from Brock about connectors)
5. Chad: select controller/drive for translational stage (preferably ELMO; getting specs from Peter; completed)
6. Kakani: update project timeline (complete)
7. Dale: check that there’s sufficient space for DeepPIV cans on benthic sled for May deployment on MiniROV (complete)
8. Alana: email Bruce to find out what his plans for MiniROV are during April cruise (completed)
9. Chad: create binder that has schematics, components for DeepPIV system (in progress)
10. Alana: check power output for science port on DR for dye injector (in progress)
11. Chad: purchase “set” components for camera housing (in progress)
12. Kakani: purchase SD card compatible with high speed recording (completed)
13. Kakani: purchase battery eliminator for Sony camera (completed)
14. [bookmark: _GoBack]Dale: follow up with Ben to resolve camera housing designs (completed; using 8 in ID titanium housing for camera)
15. Kakani: drop off couplers to Dale (complete)
16. Alana: complete two budget transfers to get our money back (completed)
17. Kakani: follow up with Larry and tell him we will pay restocking fee (completed)
18. Kakani: follow up with Mike at Edgertronic and ask about turn around time (completed)
19. Kakani: test Sony A7SII camera (see below)
20. Kakani: differences between Sony A7S and A7Sii
21. Alana: discuss with Steve about Sony A7S
22. Kakani: talk to LaserGlow about the fiber optics assembly with Dale
23. Alana/Chad: rewire dye injector motor
24. Kakani: provide dimensions for DeepPIV configuration

2016ish
1. Dale: make camera settings data available for VARS (in progress)
2. Dale: change color (flashing red) when delta exceeds some value (in progress)

Notes:
AC solution for power interface to other vehicles
In camera housing: camera, lens power source, just add power module
Injector power and controller as stand-alone unit from DeepPIV

Kakani: test the following for sony a7sII
	High speed recording
	Trigger high speed recording from software
	Change record settings from software
	FOV size for camera/lens 
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