Here’s a summary of our action items:
 
1. Chad: electrical schematic/diagram for high speed camera to larger vehicles (change of camera from high-speed to high-sensitivity in design; get model information from Alana; in progress)
2. Chad: create binder that has schematics, components for DeepPIV system (in progress)
3. Alana: check power output for science port on DR for dye injector (completed; 24V and 2A, 110AC and 10A)
4. Chad: purchase “set” components for camera housing (completed)
5. Kakani: test Sony A7SII camera (see below; completed)
6. Kakani: differences between Sony A7S and A7Sii (completed)
7. Alana: discuss with Steve about Sony A7S (completed)
8. Kakani: talk to LaserGlow about the fiber optics assembly with Dale (completed)
9. Alana/Chad: rewire dye injector motor (in progress)
10. Kakani: provide dimensions for DeepPIV configuration (completed)
11. Kakani: retest A7S with USB and HDMI connected while recording in XAVCS
12. Chad: follow up with DMO about GigE characterization
13. Chad: block diagram for laser+controller housing
14. Chad: wiring diagram for dye injector
15. Kakani: redo calculations using 75 deg optic
16. [bookmark: _GoBack]Jon: find components in controller can in vault and draw up new laser+controller can

2016ish
1. Dale: make camera settings data available for VARS (in progress)
2. Dale: change color (flashing red) when delta exceeds some value (in progress)

Notes:
AC solution for power interface to other vehicles
In camera housing: camera, lens power source, just add power module
Injector power and controller as stand-alone unit from DeepPIV

Kakani: test the following for sony a7sII
	High speed recording
	Trigger high speed recording from software
	Change record settings from software
	FOV size for camera/lens 
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