Here’s a summary of our action items:
 
1. Chad: electrical schematic/diagram for camera to larger vehicles (change of camera from high-speed to high-sensitivity in design; get model information from Alana; in progress)
2. Chad: create binder that has schematics, components for DeepPIV system (in progress)
3. Alana/Chad: rewire dye injector motor (in progress)
4. Kakani: retest A7S with USB and HDMI connected while recording in XAVCS (completed)
5. Chad: follow up with DMO about GigE characterization (completed)
6. Chad: block diagram for laser+controller housing (completed)
7. [bookmark: _GoBack]Chad: wiring diagram for dye injector (in progress)
8. Kakani: redo calculations using 75 deg optic (completed)
9. Jon: find components in controller can in vault and draw up new laser+controller can (in progress)
10. Chad: get pin out for camera housing and discuss cabling/ports for housing
11. Chad: specify connectors for camera and laser housing
12. Dale: follow up with Brock about fiber optic penetrators
13. Dale: purchase ELMO for DeepPIV project
14. Kakani: retest new A7S and return Steve’s camera
15. Kakani: purchase spare line optics (x2)

2016ish
1. Dale: make camera settings data available for VARS (in progress)
2. Dale: change color (flashing red) when delta exceeds some value (in progress)

Notes:
AC solution for power interface to other vehicles
In camera housing: camera, lens power source, just add power module
Injector power and controller as stand-alone unit from DeepPIV
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