1. The current version of the DeepPIV v.4 LabView software can be found in the MBARI bitbucket repository: https://bitbucket.org/mbari/dpiv4/
2. The version of the software which runs the camera, injector, and laser is the branch “SonyCoherentGUI”. The master just operates the laser. I will change this when the software is finished.
3. You will need an account on Atlassian.com to access the repository. You can clone the repository to get a local copy of the latest version. I use Sourcetree which allows has a user interface for push/pull/cloning. But you can just do a clone request on the command line.
4. To run the software you need a LabView version 18. 
5. Install the LabJack UD drivers for windows
6. You need the following libraries added to labview (you can use the package manager to load them): LabJack LJUD, OpenG (for timer fcns), NI GOOP (not positive on this one)
7. Open the Project DeepPIV4MultiQ.lvproj
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