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Interrupt Priorities
	7
	PWR_FAIL

	6
	

	5
	Modbus over SPI

	4
	UARTS

	3
	Modbus Timers

	2
	RTC on INT4

	1
	FreeRTOS Kernel, Ticker

	0
	



FreeRTOS.h:  
configMAX_SYSCALL_INT_PRIO  is set to 5.  This allows the hardware interrupt handlers to use the FromISR functions.  See http://www.freertos.org/a00110.html#kernel_priority
configKERNEL_INTERRUPT_PRIORITY is set to 1, per the “Kernel” entry above.
[bookmark: _GoBack]PIC32 Timers
	1
	FreeRTOS ticker (FreeRTOS/PIC32/port.c)

	2
	Modbus  SPI

	3
	Modbus UARTs

	4, 5
	Unused


FreeRTOS Task Priorities
	5
	Shutdown Task

	4
	Kernel Timer Task

	3
	Interrupt Completion Threads

	2
	Oasis Drivers

	1
	Oasis Scheduler

	0
	Idle



FreeRTOS.h:  configTIMER_TASK_PRIORITY = 4
