	YEAR
	2014
	2015
	2016
	2017 and beyond

	Monitoring of upper ocean parameters at Sta. MB and Sta. M
	Monthly with ship cast (Sta.  MB)
	Development of 300 m water-sampling LRAUV complete
	
	Bi-weekly monitoring by 300m water-sampling LRAUV, profiling and wave gliders, and data processing at Sta. MB
	Bi-weekly monitoring by 300m water-sampling LRAUV, profiling and wave gliders, and data processing at Sta. MB and Sta. M

	
	
	
	Develop 300m LRAUV docking for power and data exchange
	
	

	Monitoring of midwater faunal community, physical and chemical parameters at  Sta. MB and Sta. M
	Monthly with ROV (Sta. MB)
	Development of imaging for AUV Dorado
	Monitoring using optical imaging AUV Dorado at 100m intervals down to 1000 m depth, and  data processing at  Sta. MB
	Monitoring using optical and acoustic imaging AUV Dorado at 100m intervals down to 1000 m depth, and  data processing at  Sta. MB and Sta. M

	Monitoring of benthic community, physical and chemical parameters at  Sta. MB and Sta. M
	Yearly with ROV (Sta. M)
	
	Monitoring using optical and acoustic imaging AUV Dorado from sea floor to 50 m above bottom, and data processing at  Sta. MB
	
	Bi-weekly monitoring using optical and acoustic imaging 4000m LRAUV from the sea floor to 50 m above bottom at Sta. MB and Sta. M, and data processing

	
	
	
	
	Begin to develop 4000m-LRAUV for full-depth optical and acoustic monitoring at both stations.
	

	
	
	
	
	Begin to develop 4000m-LRAUV with docking capabilities for both data and power exchanges.
	

	Sediment traps and time-lapse camera mooring, servicing, and data processing at Sta. MB and Sta. M
	Annual servicing Sta. M
	Install existing mooring of two sediment traps and time-lapse camera- Sta. MB
	Sedimentation and sea floor monitoring with annual servicing of moorings, at both stations. Data analysis automated at Sta. MB and Sta. M

	Water column monitoring system
	
	
	Develop mooring based instrumentation to provide continuous monitoring of water column (low-cost cameras, RDI acoustics, SES) with LRAUV data and power exchanges through docking stations
	Continuous monitoring of water column (low-cost cameras, RDI acoustics, SES) with LRAUV data and power exchanges through docking stations

	Data management and acquisition system for MBARI time-series data
	Development complete
	Used internally for data management and analysis
	Data also available to public domain
	

	Sediment trap (500m) w/extended mooring at Sta. M
	
	
	Purchased and installed
	Sedimentation monitoring with annual servicing of mooring. Data analysis automated

	VARS routines for processing AUV images from midwater and benthic transects
	
	
	Development complete
	
	[bookmark: _GoBack]VARS used for processing AUV images from midwater and benthic transects

	
	
	
	
	
	

	Export time-series instrumentation, data management system
	
	
	
	
	
	
	Exported instrumentation and data management system
	Put time series data in public domain

	TOTAL SHIPTIME (d)  30 
	Data collection
	
	
	

	20
	
	Concurrent data collection and technology calibration
	
	

	10
	Servicing
	Servicing
	Servicing
	Servicing


Table 1. Schedule for development and implementation of integrated time-series program
