
[image: S:\Documents\Testing\Syntactic\IMG_6433.JPG]Last year we deployed 28 blocks that weighed 163 lbs in air, and -162 lbs in water.  It was ballasted with one lead brick and two lead disks that weighted ~ 50 lbs.  The two Novatech beacons and the homer were about 8 lbs and the bail as another 2 lbs.   Package should be ~100 lbs buoyant. A large mushroom anchor was added to hold it down.  Not sure how much the mushroom weighted
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[bookmark: _GoBack]2016 Test: 28 blocks total 4 stacks of 7 mounted on old elevator



 (28) Blocks to be mounted to the old elevator
Blocks weigh 221 lbs in air 
Blocks weigh -195 lbs in water






Ballast and beacons[image: ]r
~60 lbs of ballast, beacons and frame

Elevator assembly is ~135 lbs buoyant and stable on the surface (195 buoyancy 60 lbs ballast) 




An anchor is needed to sink and hold the elevator down at about 2:1, so 2*135 lbs=270 . 
 Anchor needs to be ~270 lbs in water.  
Use (2) double rail assemblies that provide 130 lbs ballast each for 260 lbs combined.
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