2/7/17
MBARI: Stereo Camera test

Test 1: Small tank 
1. Configuration 
a. ISO: 500
b. F8 aperture
c. 7.5 degree tow in
d. 1/125th shutter speed (originally set to 1/100, but changed before photos taken)
e. Small tank with calibration board only at 0.5 meters from camera
f. Two lights
2. One set of images taken with these settings (top and bottom)
3. 5 second video taken with these settings 
4. 5 second video: same settings. This time a fish target was placed in the tank
5. Second set of still images taken using Copper Rockfish target (27cm long)
Test 2: Large tank
1. Configuration 
a. ISO 500
b. F8 aperture 
c. 7.5 degree tow in
d. 1/10 second shutter speed
e. Distance from target is 1.5 meters
f. Lower camera is ~39.5 cm above bottom of tank (bottom of calibration board)
2. Still taken without fish: just board
3. Stills with fish (Starry Rockfish: a darker and more cryptic species to ID)
a. Top
b. Middle 
c. Bottom 
4. 5 second video: using fish target moving about the frame
5. Determined that one of the lights was not turned on, and so repeated large tank tests starting with video
6. 5 seconds of video using the Starry Rockfish target
a. Target moved about the frame
7. Set of three photos with Starry Rockfish target
a. Top
b. Middle
c. Bottom
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