· Features
· Quad, Picture in Picture, Full Screen, and Custom display modes (Custom Display Mode: the size, position and selection of any or all windows are customizable)
· 2- and 3-source viewing is possible with this method
· Maintain input aspect ratio if desired-no stretching necessary
· Layer display windows and adjust transparency of each video source display
· Independent video in to video out resolution
· Supports 2K resolution 2048x1080, HDTV resolutions to 1080p, and computer resolutions to 1920x1200
· HDMI features supported:
· Inputs: 24-, 30-, and 36-bit xvYCC, sRGB, and YCbCr
· Outputs: 24- and 30-bit sRGB
· Four-channel non-mixing or one channel mixing stereo with 16-, 20-, or 24-bit uncompressed PCM audio
· Bandwidth up to 165 MHz
· Inputs: 2.25 Gbps
· Output: 2.0625 Gbps
· HDCP compliant
· Fluid, real-time video performance with 60 frames per second (fps) in all four quadrants
· Zoom, pan, and crop the image from any source to focus on key areas
· Switch audio independently of video from connected HDMI sources (e.g. source 1 and source 2 video are active while only source 3 audio is active)
· Multiple audio sources can be simultaneously active in any display mode or preset layout
· Adjustable audio gain with VU level indicators for each input channel
· A customized text label can be added for each video window to provide easy input identification (UMD)
· Any DVI source or display can be connected by using the DVI-HD-xx-MM cable (not included)
· Use DVIA-HD-CNVTR-LC or DVI-HD-CNVTR DVI + Audio to HDMI Converters to pass and independently switch audio signals to the multiviewer
· Control the multiviewer through Ethernet, RS232 serial port, on screen display (OSD), front panel buttons, or IR remote
· Cascade multiviewers to display video from any number of video sources on one screen
· Each video source in the cascade can be controlled directly from the Web Server graphical user interface under Custom Mode Settings
· Backup and restore multiviewer configurations
· Supported output resolutions can be selected or set to auto detect optimal resolution from the monitor's EDID
· Desktop unit
 
· Specifications
· Video Input
· Four female HDMI connectors.
· Supported video input resolutions:
· 2K Cinema (2048x1080 @ 60Hz).
· HDTV resolutions to 1080p.
· Computer resolutions to 1920x1200.
· Supports digital HDMI devices, such as DVD/Blu-ray players, satellite receivers and HDTV tuners.
· Multiplatform support: Windows 2000/XP/Vista/7/8, Windows Server 2000/2003/2008, Solaris, Linux, FreeBSD, and MAC OS 9/10.
· A DVI source can be connected by using the DVI-HD-xx-MM cable (not included). The cable does not pass audio to the multiviewer.
· Video Output
· One female HDMI connector.
· Supported video output resolutions:
· 2K Cinema (2048x1080 @ 60Hz).
· HDTV resolutions to 1080p.
· Computer resolutions to 1920x1200.
· HDMI-embedded audio switching (four-channel stereo, non-mixing or one-channel stereo, mixing).
· A DVI display can be connected by using the DVI-HD-xx-MM cable (not included). The cable does not pass audio to the display.
· Protocols
· HTTP, HTTPS.
· TCP/IP, DHCP, UDP, ARP.
· IPV4.
· Power
· 110 to 220 VAC at 50 or 60Hz via country-specific AC adapter.
· Power consumption: 10W
· Environmental
· Operating temperature: 32 to 122°F (0 to 50°C).
· Storage temperature: -22 to 140°F (-30 to 60°C).
· Operating and storage relative humidity: 17 to 90% non-condensing RH.
· Dimensions WxDxH (in): 7.35x4.98x1.09 (187x126x28 mm).
· Regulatory Approval: CE, RoHS, TAA compliant.
 
· Item Includes
· 1x SPLITMUX-HD-4RT multiviewer
· 1x country-specific power cord
· 1x DB9 female to RJ45 female adapter
· 1x 5-ft CAT5e super flat patch cable
· 1x IR remote control with two AAA batteries
· 1x CD that contains the manual and NTI Discovery Tool
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