Sony Multi / Micro USB Terminal

M1: Vbus (+5V, 2A max)
M2: USBD-
M3: USBD+
M4: USB_ID
M5: GND

M6: +3.1V (for LANC_DC)
M7: reserved
M8: LANC_SIG
M9: reserved
M10: SELECT (resistor to M6 or M14)
M11: Audio R Out / Activate Camera / Focus
M12: Audio L Out / Release Shutter
M13: Composite Video Out
M14: GND
M15: reserved

	U1
	VBUS (+5V, max 2A)

	U2
	USB D-

	U3
	USB D+

	U4
	USB ID

	U5
	GND_USB

	—
	

	M10
	+3.3V (MULTI_DC)

	M09
	reserved

	M08
	“UART_TX” / “LANC_SIG” (At A6000 it seems to be UART; No LANC!)

	M07
	“UART_RX” / “BOOT_IN” (At A6000 it seems to be UART; No Bootloader/Debug)

	M06
	SELECT (resistor against M01 or M09 for selecting Multiport functionalitites/protocol)

	M05
	Short to ground to focus, Audio R out

	M04
	Short to ground to take image, Audio L out

	M03
	Maybe composite video out (no AV-out at A6000 known to me!)

	M02
	GND (identical to GND_USB)

	M01
	Power_On/Off (short to GND)







· 1: "VBUS" - 5V-Eingangsspannung vom USB-Host
· 2: "D-" - USB-Datenleitung (negativ)
· 3: "D+" - USB-Datenleitung (positiv)
· 4: "USB_ID" - für USB-OnTheGo
· 5: "GND" - in der Kamera mit Pin 14 ("AV_GND") verbunden
· 6: "D_3.1V" / "LANC_DC" - Ausgang für 3.1 bis 3.3V Spannung
· 7: "XRESET_REQ" - Eingang für Reset-Anfrage
· 8: "UART_TX" / "LANC_SIG" - optionaler Ausgang für serielle Schnittstelle (Debug) oder LANC
· 9: "UART_RX" / "BOOT_IN" - optionaler Eingang für serielle Schnittstelle (Debug) und Bootloader
· 10: "AD_JACK_IN" - Analoger Eingang für Widerstand zur Erkennung des angeschlossenen Kabel-/Zubehörtyps
· 11: "LINEOUT_R" / "XAE_LOCK_SW" - optionaler Audioausgang (rechts, in der Kamera über Kondensator entkoppelt) und/oder Eingang für Auslöser (1. Stufe) im Fotomodus der Kamera (und mit richtigem Widerstand an AD_JACK_IN)
· 12: "LINEOUT_L" / "XSHUT_SW" - optionaler Audioausgang (links, in der Kamera über Kondensator entkoppelt) und/oder Eingang für Auslöser (2. Stufe) im Fotomodus der Kamera (und mit richtigem Widerstand an AD_JACK_IN)
· 13: "VIDEO" - optionaler Composite-Video-Ausgang
· 14: "AV_GND" - in der Kamera mit Pin 5 ("GND") verbunden
· 15: "XPWR_ON" - Eingang für externen ON/OFF-Taster (gegen GND)
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Figure 1: Multiport connector pin numbers
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Figure 2: Multiport connector pin names

Pinout according to Figures 1 and 2:

USB
A1  Vbus (+5V, 2A Max)
A2  USB Data -
A3  USB Data +
A4  USB ID
A5  Gnd

Multiport
1  +3.1V (LANC DC)
2  Reserved
3  UART Tx
4  UART Rx
5  Select (Resistor to pin 1 or 9)
6  Audio Out R / Focus
7  Audio Out L / Shutter
8  Composite Video Out
9  Gnd (same as USB Gnd)
10 Camera Power On/Off






















[image: ]
Figure 3: Sony Multiport 10 pin signals
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Figure 4: Sony Multiport USB signals
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