ST switch settings   PA500/6 and PA 200/20 standard Version 9 software
	Altimeter choice – complete one column only

	Material/depth/style
	Connector
	PA500/6
	PA200/20
	LPA200/10

	Check one only
	Delrin 700m R/A  
	TIL 6 way
	   Ab-D-A|_|S6164
	   Ab-D-A|_|S6868
	

	
	Delrin 700m Str.
	TIL 6 way
	D-D-A|_|S2133
	D-D-A|_|S2135
	

	
	Alum. 4000m R/A
	TIL 6 way
	   Ab-A-A|_|S4807
	   Ab-A-A|_|S3447
	

	
	Alum. 4000m Str.
	TIL 6 way
	A-A-A|_|S5303
	A-A-A|_|S4678
	A-A-A|_|S4519

	
	S/S 4000m Str.
	TIL 6 way
	S-S-S|_|S2125
	[bookmark: Check16]S-S-S|_|S2127
	

	
	S/S 6,800m Str.
	XSG-6-BCL
	S-S-S|_|S5301
	[bookmark: Check17]S-S-S|_|S5300
	Special Whip Req.

	
	Special connector
	|_|
	? ? ?
	|_|

	one only
	Pinouts
	Tritech Standard
	|_|

	
	
	Non Standard*
	|_|

	Check one only
	Timeout range
	200m
	
	
	|_|

	
	
	100m
	
	|_|
	

	
	
	50m
	|_|
	|_|
	

	
	
	10m
	|_|
	
	

	Check one only
	Analog scaling
(if required)
	0-200m
	
	|_|

	
	
	0-100m
	
	|_|
	

	
	
	0-50m
	|_|
	|_|
	

	
	
	0-30m
	|_|
	|_|
	

	
	
	0-20m
	|_|
	|_|
	

	
	
	0-15m
	|_|
	|_|
	

	
	
	0-10m
	|_|
	|_|
	

	
	
	0-5m
	|_|
	|_|
	

	
	
	0-2m
	|_|
	|_|
	

	Power input/analog/serial output  - complete one column only

	
	Power supply
(10.5 to 28VDC)
	Specify actual supply
          VDC
	Note
.
TTL & CURRENT LOOP DO NOT HAVE A SERIAL OUTPUT (232/485)

	Check one only
	Analogue  Voltage Output
	none 
	[bookmark: Check25]               |_|
	

	
	
	5V
	[bookmark: Check29]               |_| 
	

	
	
	10V
	[bookmark: Check30]               |_| supply must be >12.5VDC
	

	Check one only
	Serial and Current Output
	none
	[bookmark: Check55]               |_|
	

	
	
	4-20mA
	               |_| supply must be >15VDC
	

	
	
	RS232
	[bookmark: Check39]               |_|
	RS485 termination

	
	
	RS485 
	               |_|
	 ?_______

	Other options

	Check one only in each row
	No return output
	Zero
	Full range
	TTL Trigger 
	

	
	
	|_|
	|_|
	[bookmark: Check62]Must be full range |_|
	

	
	Mode
	Free run
	Z Interrogate 
	[bookmark: Check60]Timeout         |_|
	Ascii address (A-H) 

	
	
	|_|
	|_|
	[bookmark: Check61]No timeout     |_|
	|_|

	
	Serial message
	xxx.xxxm<CR><LF>
	xxx.xxm<CR><LF>
	xx.xxxm<CR><LF>
	Xxx.xxxm<CR><LF>

	
	
	|_|
	|_|
	|_|
	Character ?___ 

	Tritech mating 
connector if used
	Straight
	Right angle
	Tail length
	

	
	|_|
	|_|
	N/A
	

	Customer 
	

	Extra notes and 
*Non Standard Pinouts
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SW1
	Mode
	6
	5
	4
	3
	2
	1
	
	Mode
	6
	5
	4
	3
	2
	1
	
	SubNode

	0
	0
	0
	0
	0
	0
	0
	DEBUG IN ZNE
	32
	1
	0
	0
	0
	0
	0
	LAN IN ZNE
	A

	1
	0
	0
	0
	0
	0
	1
	DEBUG FR ZNE
	33
	1
	0
	0
	0
	0
	1
	
	B

	2
	0
	0
	0
	0
	1
	0
	DEBUG IN MNE
	34
	1
	0
	0
	0
	1
	0
	
	C

	3
	0
	0
	0
	0
	1
	1
	DEBUG FR MNE
	35
	1
	0
	0
	0
	1
	1
	
	D

	4
	0
	0
	0
	1
	0
	0
	3P3 IN ZNE
	36
	1
	0
	0
	1
	0
	0
	
	E

	5
	0
	0
	0
	1
	0
	1
	3P3 FR ZNE
	37
	1
	0
	0
	1
	0
	1
	
	F

	6
	0
	0
	0
	1
	1
	0
	3P3 IN MNE
	38
	1
	0
	0
	1
	1
	0
	
	G

	7
	0
	0
	0
	1
	1
	1
	3P3 FR MNE
	39
	1
	0
	0
	1
	1
	1
	
	H

	8
	0
	0
	1
	0
	0
	0
	2P3 IN ZNE
	40
	1
	0
	1
	0
	0
	0
	LAN IN MNE
	A

	9
	0
	0
	1
	0
	0
	1
	2P3 FR ZNE 
	41
	1
	0
	1
	0
	0
	1
	
	B

	10
	0
	0
	1
	0
	1
	0
	2P3 IN MNE
	42
	1
	0
	1
	0
	1
	0
	
	C

	11
	0
	0
	1
	0
	1
	1
	2P3 FR MNE
	43
	1
	0
	1
	0
	1
	1
	
	D

	12
	0
	0
	1
	1
	0
	0
	3P2 IN ZNE
	44
	1
	0
	1
	1
	0
	0
	
	E

	13
	0
	0
	1
	1
	0
	1
	3P2 FR ZNE 
	45
	1
	0
	1
	1
	0
	1
	
	F

	14
	0
	0
	1
	1
	1
	0
	3P2 IN MNE
	46
	1
	0
	1
	1
	1
	0
	
	G

	15
	0
	0
	1
	1
	1
	1
	3P2 FR MNE
	47
	1
	0
	1
	1
	1
	1
	
	H

	16
	0
	1
	0
	0
	0
	0
	V3BATHY IN ZNE
	48
	1
	0
	0
	0
	0
	0
	DLE IN ZNE
	0

	17
	0
	1
	0
	0
	0
	1
	NMEA FR ZNE
	49
	1
	1
	0
	0
	0
	1
	
	1

	18
	0
	1
	0
	0
	1
	0
	NMEA FR MNE
	50
	1
	1
	0
	0
	1
	0
	
	2

	19
	0
	1
	0
	0
	1
	1
	TSS FR ZNE
	51
	1
	1
	0
	0
	1
	1
	
	3

	20
	0
	1
	0
	1
	0
	0
	TSS FR MNE
	52
	1
	1
	0
	1
	0
	0
	
	4

	21
	0
	1
	0
	1
	0
	1
	
	53
	1
	1
	0
	1
	0
	1
	
	5

	22
	0
	1
	0
	1
	1
	0
	
	54
	1
	1
	0
	1
	1
	0
	
	6

	23
	0
	1
	0
	1
	1
	1
	
	55
	1
	1
	0
	1
	1
	1
	
	7

	24
	0
	1
	1
	0
	0
	0
	
	56
	1
	1
	1
	0
	0
	0
	DLE IN MNE
	0

	25
	0
	1
	1
	0
	0
	1
	
	57
	1
	1
	1
	0
	0
	1
	
	1

	26
	0
	1
	1
	0
	1
	0
	
	58
	1
	1
	1
	0
	1
	0
	
	2

	27
	0
	1
	1
	0
	1
	1
	
	59
	1
	1
	1
	0
	1
	1
	
	3

	28
	0
	1
	1
	1
	0
	0
	
	60
	1
	1
	1
	1
	0
	0
	
	4

	29
	0
	1
	1
	1
	0
	1
	DIGTRIG MNE
	61
	1
	1
	1
	1
	0
	1
	
	5

	30
	0
	1
	1
	1
	1
	0
	DIGTMO MNE
	62
	1
	1
	1
	1
	1
	0
	
	6

	31
	0
	1
	1
	1
	1
	1
	SONV3
	63
	1
	1
	1
	1
	1
	1
	
	7



IN = INTERROGATE		MNE = MAX NO ECHO		0 = OFF
FR = FREE RUN			ZNE = ZERO NO ECHO		1 = ON

SW2
	SW2-1
	LOCKOUT
	
	SW2-4
	SW2-3
	SW2-2
	Analog scaling

	1
	500kHz/10m only
	
	1
	1
	1
	2m

	0
	Standard
	
	1
	1
	0
	5m

	
	
	
	1
	0
	1
	10m

	SW2-6
	SW2-5
	RANGE/FREQ
	1
	0
	0
	15m

	1
	1
	500kHz/10m
	0
	1
	1
	20m

	1
	0
	500kHz/50m
	0
	1
	0
	30m

	0
	1
	200k/Hz/50m
	0
	0
	1
	50m

	0
	0
	200kHz/100m
	0
	0
	0
	100m


		Notes
		For serial control (non LAN settings)	Interrogate character =Z
		Switch from interrogate to free run = F	Switch from free run to interrogate = Z (RS232 only)
		
		For ASCII LAN control	Interrogate = address character (e.g. A)
		Interrogate all = *  with 26msec delay between replies      For DIGTMO mode timeout=200msec
