Fault Detection Meeting
11/28/2018
Attendees
Matt, Jon, Eric, Scott
Jon
· Pressure test: pass  (9 cycles to 450m w/ 1 hour hold).
· Long nose parts: the PO will be issued this month.
· Need to add a heat sink.
Scott
· PCBs: all done.
· connectors/cables: all are in-house.
· testbed connectors: will order a set of connectors/cables s/t we can test on the testbed independently of the vehicle.
Eric
· December availability is limited to week of Dec 3-7.
· Will set aside 2 blocks of 1 week each in the Jan/Feb time frame dedicated exclusively to the project.
MK
· We'll push integration as far as we can w/the testbed:
· Connect the chassis.
· [bookmark: _GoBack]Test the noise level.
· Test the comms.
· Test the SW components:
· data acquisition
· TDMS logging of raw data
· pause/resume
· AHRS
· pre-processing
· fault-detection
· fault-isolation
· transient-rejection state machine
· LCM
· HDF5
· Test the nominal case.
· Test the overload case.
· Test the post-processing tools.
· Once vehicle is ready and S/W1.0 are released, we'll do:
· test protocol sequence through mission file
· LCM messaging
· Next: hardening tests
· Runs of 1h without fail.
· Next: tank testing.
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