MiVEGAS TAILCONE FINISHWORK						5/23/16

1. Grind out a 0.05” relief on reinforced areas at the side fin shaft holes, room for spacers
2. Enlarge hole to oval shape for antenna wires, use shoe for guide
3. Enlarge holes (4) for ant mast mount to .23”, easier fitting.
4. Make slot for ¼-20 aft ant mount.
5. Match drill 0.09” hole for Argos ant pass thru
6. Abraid area aft of antenna hole for Argos radio to be bonded to inner shell, use flexible epoxy
7. If necessary, Slightly enlarge all 8 mount holes for tailcone 
8. Seal all abraided, cut  areas to seal C/F.  low viscosity Epoxy
9. [bookmark: _GoBack]Reinforcing guide strips and screw mounts of G-10 may be bonded on as well
