LRAUV VB Controller Modification Instructions

Required to improve resolution of the 10k potentiometer sensing. 
1.) Remove  R30, R32, R34, R35

2.) Short across R26, R27, R28, R29

3.) Replace R31 and R33 with 0805 5.23K 1% resistor
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