LRAUV BUILD5 CRITICAL REVISIONS AND FIXES!
⎕ 1. Fix erroneous wiring on drop weight connector J33.
⎕ 2. Fix erroneous wiring on NAL9602 connector J14.
⎕ 3. Check CradlePoint Ethernet wiring. External LAN connector goes to Starboard side connector when in installed position (Ethernet WAN connection).
[bookmark: _GoBack]⎕ 4. Check AHRS wiring. WHOI/DHS vehicle had swapped polarity and swapped wires with USBL comms. Change AHRS LCB to TTL logic level from EIA232.
