Tethys Load Control/Analog Board
Configuration Sheet

For Rev 1.1 LCB-Analog
 8 Aug 2012
ecm
fork from LCB Config Sheet
Board S/N:   





  Voltage: 




  
Application (connected device):  









Configuration by:  




  Date:  





Target Vehicle:




  Program: 





Custom Analog Configuration:
Bridge Drive or sensor power:

R39
(bridge drive Vref divider)

10k/2.0k default


  

R40
(bridge drive current shunt)

680 ohm default


  

Input Divider:
R43 & R46 (low side):

no-stuff default




R41 & R48 (high side): 

10.0 k
 default




C31 (low pass):


0.22uF default





Diff Amp:
R44 & R45 (gain)


10k/1k default





U19 (diff amp pair)


LT6014 default




Custom Aux Sensor (e.g. Temperature) Configuration:
Function:  












R51 (input divider):


no-stuff default




R52 (input gain):


no-stuff default




