
8.	Defaults for E0_Int = -0.4 and E0_ext = -1.3   Remove TC_Offset
a.	DONE


Configuration Menu--SeaFET/SeapHOx v3.2.0 SEAFET
1 -- Set Clock
2 -- Change File Name
3 -- Set Deployment Parameters
4 -- Enter pH Sensor Calibration Coefficients
5 -- Calculate pH Sensor Calibration Coefficients
6 -- Change Baud Rate
7 -- Config Data Fields
9 -- Exit to Main Menu
Enter Selection [9]: 4

Enter E0_int @ 25 C [-0.400000]: 5
Enter number between -2 and 2 (ex. -0.4)


Enter E0_int @ 25 C [-0.400000]: -0.4

Enter E0_ext @ 25 C [-1.320000]: 5
Enter number between -2 and 2 (ex. -1.3)


Enter E0_ext @ 25 C [-1.320000]: -1.3

*****Calibration Coefficients Saved*****


-------------------------------------------------------------------------

9.	If ‘Sleep’ from main menu and hit a key, should come back to main menu (if sample rate is 0, it does not)

Configuration Menu--SeaFET/SeapHOx v3.2.0 SEAFET
1 -- Set Clock
2 -- Change File Name
3 -- Set Deployment Parameters
4 -- Enter pH Sensor Calibration Coefficients
5 -- Calculate pH Sensor Calibration Coefficients
6 -- Change Baud Rate
7 -- Config Data Fields
9 -- Exit to Main Menu
Enter Selection [9]: 3


Sample aligned to hour? (Y/N) [N]?


Enter sample period [10] sec: 0

Sample period is zero - polled mode
Sample period now 0 sec.


Enter pH sample average [10] samples:

Enter pump on time [0] sec:

Enter low battery_voltage (10.5 V for SeapHOx, 5.5 V for SeaFET) [10.5 V]:


Output mode menu
1 -- Normal  (Data only)
2 -- Verbose (Data with prompts)
Enter Selection [1]:



Configuration Menu--SeaFET/SeapHOx v3.2.0 SEAFET
1 -- Set Clock
2 -- Change File Name
3 -- Set Deployment Parameters
4 -- Enter pH Sensor Calibration Coefficients
5 -- Calculate pH Sensor Calibration Coefficients
6 -- Change Baud Rate
7 -- Config Data Fields
9 -- Exit to Main Menu
Enter Selection [9]:


System data stored.  -- Press enter to bring up main menu


413 / 24.5  = 16.8 australia
5270 / 324  = 16.3 tpp us
573 / 37    = 15.5 tpp canada
45 / 5.3    = 8.5 tpp norway
9839 / 1410 = 7.0 tpp china
2467 / 1340 = 1.8 tpp india






Main Menu--SeaFET/MFET v3.2.0 SEAFET  -- Will deploy in 30 seconds
1 -- Configure
2 -- Deploy
3 -- Test
4 -- Sleep
5 -- Files
Enter Selection: 4



Main Menu--SeaFET/MFET v3.2.0 SEAFET  -- Will deploy in 30 seconds
1 -- Configure
2 -- Deploy
3 -- Test
4 -- Sleep
5 -- Files
Enter Selection:

Sleeping...hit any key to wake