Readme SeaFET_SeapHOx_V3.0

This program is an offshoot from SeaFET_SeapHOx_V3.0. 

The purpose of this program is to operate the SeapHOx controller as a pH data logger in the laboratory. The controller is polled for data using a laptop, and it displays voltages/data that
are only related to the pH meausrements. Currently it can return necessary data in ~3 seconds and go back to sleep. 

YT added ability for program to produce std dev for the voltage measurements, and commented out other functions in the deployment loop, such as turning on pumps and communciating with peripheral devices.


