Updates to Spray
mFET firmware updates
· Report Ik as nA (150uv = 1nA)
· Report Ib as nA (1mV = 1nA)
· Measure bias battery + and – (how much extra time will this cost?)
· Question to all: Should we install a single Li D cell instead? That will last > 5 years or so of continuous use, so we can just forget about it, rather than replacing AA every year.
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Spray firmware updates
· Why were different firmwares loaded onto 029 and 034 again?
· make pump on 2 minutes before ascent consistent across all firmwares
· For sat files, multiply std devs by 1000 so they report as mV, rather than V.
· Can we send back an extra decimal precision? 
· 
