Steps needed for GliderVIZ

Update parameters
· HTML file to update X and Y variables in GliderVIZ is \\sirocco/wwwroot/chemsensor/gliderviz.htm
· Update the list 
· Also need to update sirocco/wwwroot/lobo/data/GliderVizdata/GliderVIZConfig.txt.
· Variables need to be listed here. 
· Variable names need to be matched exactly between the html and config file
For a New Mission:
· In update_GliderVIZ_sat.m, change ‘missionname’ and ‘satfname’ in L15-22.
· Create folder in dropbox/spray pH/Deployments/MISSIONNAME/sat_files
· IN this folder download the first .sat file from npzd server. If there’s no sat file that exists to start with, update_GliderVIZ_sat.m won’t run.
· In: dropbox/spray pH/Deployments/MISSIONNAME, copy cal_MISSIONNAME.m. This holds calibration coefficients for the DSD.
· In \\Sirocco/wwwroot/lobo/data/GliderVizData, update GliderVIZConfig.txt by adding the text file for the current mission (i.e. MISSIONNAMERT.TXT).
· Update Sirocco/wwwroot/chemsensor/GliderViz.htm to include current new mission. 


[bookmark: _GoBack]Batch file (updateGliderVIZdata.bat) gets run on top of the hour through task scheduler. 
