To dos before next deployment


· Check SD card for ADC counts for fluorometer 
· Change output of pH controller to match 029 output (parsing issue)
· Upload firmware to measure both up/down.
· DONE 9/1/2020
· Swap out pH sensor to SBE-pcomp prototype
· DONE end of AUG/2020
· Put in tank, get cal for pH + O2
· Store full resolution pH data on CF card
· [bookmark: _GoBack]Not done this time
