How to enable Agilent 82357B USB/GPIB interface with Labview
Note: If you do this, this computer will no longer be able to use the 8453 using the Agilent software

TO use the 82357B, you need to enable NIVISATulip.dll and NI488.2 from within the Keysight (or Agilent) libraries.
Directions are taken from NI help websites:
· http://digital.ni.com/public.nsf/allkb/F7C187DBF09EBE1186256F550065BD32
· http://digital.ni.com/public.nsf/websearch/3B3626D9C1F999218625694200791AD7?OpenDocument
Enabling NI488.2 
1. Download Keysight Connection Expert (Agilent Connection Expert is outdated)
a. Can be downloaded from:
http://www.keysight.com/main/software.jspx?cc=US&lc=eng&nid=-536900526.697048.02&id=2175637&pageMode=CV
b. Restart computer
2. Under the Settings tab, select Options»Keysight 488 Options.
3. Check Enable Keysight GPIB cards for 488 programs.
4. Restart computer
Enabling NIVISATulip.dll
· Note: you need to have installed NI-VISA already. Also, you need to have installed Keysight before this, so the driver for the 82357B is obtained.
· Open NI-MAX
· Go to tools -> NI-VISA -> VISA options…
· Once the VISA Options screen appears, select Passports in the tree view (My System » General Settings » Passports). Enable the NiVisaTulip.dll by placing a check mark in the box beside it and then click on the Save button. You will need to restart MAX for the setting to take effect. Once MAX is restarted, you will be able to access your third-party GPIB boards and give them VISA aliases under My System » Devices and Interfaces » Miscellaneous VISA Resources
Configure GPIB
· Open Keysight Connection Expert
· Go to settings (or three vertical dots) on the GPIB-USB tab on the left, and choose edit…
· Set Visa interface ID to GPIB0, GPIBaddress to 30, SICL Interface ID to hp82341, and uncheck the auto-discover instruments (these instructions are from the “Installation Guide” for the Agilent 8453, Section 6). Press OK.
· Press
· GPIB should be configured to be used with LabView. 
· GPIB address in Labivew should be: GPIB0::25::INSTR
· 25 is the address for the instrument. This is configurable using the 8 switches on the back side of the 8453. Refer to table 5 and 6 in the “Installation Guide” in section 6 for address ID and switches. 
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