MinipHOX Pinout

Bulkhead (6pin) (MCBH-6-MP SS)
Terminate to a 4-pin Harwin  (Data in/out in reference to the microcontroller)
4-pin Harwin header		SubConn wet-matable pin/wire  #
1: (Data IN) --------------------	2
2: (Data OUT)------------------	1
3: -------------------------------	4
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[bookmark: _GoBack]Serial Cable (Same as SeapHOx)

Pig tail cable P/N: MCIL-6-FS (2’ pigtail)
Terminate cable to DB9 (Female)
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DB9(F)	MCIL-6-FS
    2		    Black (pin 1)
    3		    White (pin 2)
    5		    Green (pin 4)
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