libftdi1 1.0

- Main Page
- Modules
- Namespaces
- Classes
- Files

- File List
- File Members

Classes | Macros | Typedefs | Enumerations | Functions
ftdi.h File Reference
`#include <stdint.h>`
`#include <sys/time.h>`

Go to the source code of this file.

## Classes
struct | ftdi_transfer_control
struct | ftdi_context
| Main context structure for all libftdi functions. More...
struct | ftdi_device_list
| list of usb devices created by ftdi_usb_find_all() More...
struct | size_and_time
| Progress Info for streaming read. More...
struct | FTDIProgressInfo
struct | ftdi_version_info

## Macros
#define | MPSSE_WRITE_NEG 0x01 /* Write TDI/DO on negative TCK/SK edge*/
#define | MPSSE_BITMODE 0x02 /* Write bits, not bytes */
#define | MPSSE_READ_NEG 0x04 /* Sample TDO/DI on negative TCK/SK edge */
#define | MPSSE_LSB 0x08 /* LSB first */
#define | MPSSE_DO_WRITE 0x10 /* Write TDI/DO */
#define | MPSSE_DO_READ 0x20 /* Read TDO/DI */
#define | MPSSE_WRITE_TMS 0x40 /* Write TMS/CS */
#define | SET_BITS_LOW 0x80
#define | SET_BITS_HIGH 0x82
#define | GET_BITS_LOW 0x81
#define | GET_BITS_HIGH 0x83
#define | LOOPBACK_START 0x84
#define | LOOPBACK_END 0x85
#define | TCK_DIVISOR 0x86
#define | DIS_DIV_5 0x8a
#define | EN_DIV_5 0x8b
#define | EN_3_PHASE 0x8c
#define | DIS_3_PHASE 0x8d
#define | CLK_BITS 0x8e
#define | CLK_BYTES 0x8f
#define | CLK_WAIT_HIGH 0x94
#define | CLK_WAIT_LOW 0x95
#define | EN_ADAPTIVE 0x96
#define | DIS_ADAPTIVE 0x97
#define | CLK_BYTES_OR_HIGH 0x9c
#define | CLK_BYTES_OR_LOW 0x0d
#define | DRIVE_OPEN_COLLECTOR 0x9e
#define | DIV_VALUE(rate) (rate > 6000000)?0:((6000000/rate -1) > 0xffff)? 0xffff: (6000000/rate -1)
#define | SEND_IMMEDIATE 0x87
#define | WAIT_ON_HIGH 0x88
#define | WAIT_ON_LOW 0x89
#define | READ_SHORT 0x90
#define | READ_EXTENDED 0x91
#define | WRITE_SHORT 0x92
#define | WRITE_EXTENDED 0x93
#define | SIO_RESET 0 /* Reset the port */
#define | SIO_MODEM_CTRL 1 /* Set the modem control register */
#define | SIO_SET_FLOW_CTRL 2 /* Set flow control register */
#define | SIO_SET_BAUD_RATE 3 /* Set baud rate */
#define | SIO_SET_DATA 4 /* Set the data characteristics of the port */
#define | FTDI_DEVICE_OUT_REQTYPE (LIBUSB_REQUEST_TYPE_VENDOR | LIBUSB_RECIPIENT_DEVICE | LIBUSB_ENDPOINT_OUT)
#define | FTDI_DEVICE_IN_REQTYPE (LIBUSB_REQUEST_TYPE_VENDOR | LIBUSB_RECIPIENT_DEVICE | LIBUSB_ENDPOINT_IN)
#define | SIO_RESET_REQUEST SIO_RESET
#define | SIO_SET_BAUDRATE_REQUEST SIO_SET_BAUD_RATE
#define | SIO_SET_DATA_REQUEST SIO_SET_DATA
#define | SIO_SET_FLOW_CTRL_REQUEST SIO_SET_FLOW_CTRL
#define | SIO_SET_MODEM_CTRL_REQUEST SIO_MODEM_CTRL
#define | SIO_POLL_MODEM_STATUS_REQUEST 0x05
#define | SIO_SET_EVENT_CHAR_REQUEST 0x06
#define | SIO_SET_ERROR_CHAR_REQUEST 0x07
#define | SIO_SET_LATENCY_TIMER_REQUEST 0x09
#define | SIO_GET_LATENCY_TIMER_REQUEST 0x0A
#define | SIO_SET_BITMODE_REQUEST 0x0B
#define | SIO_READ_PINS_REQUEST 0x0C
#define | SIO_READ_EEPROM_REQUEST 0x90
#define | SIO_WRITE_EEPROM_REQUEST 0x91
#define | SIO_ERASE_EEPROM_REQUEST 0x92
#define | SIO_RESET_SIO 0
#define | SIO_RESET_PURGE_RX 1
#define | SIO_RESET_PURGE_TX 2
#define | SIO_DISABLE_FLOW_CTRL 0x0
#define | SIO_RTS_CTS_HS (0x1 << 8)
#define | SIO_DTR_DSR_HS (0x2 << 8)
#define | SIO_XON_XOFF_HS (0x4 << 8)
#define | SIO_SET_DTR_MASK 0x1
#define | SIO_SET_DTR_HIGH ( 1 | ( SIO_SET_DTR_MASK << 8))
#define | SIO_SET_DTR_LOW ( 0 | ( SIO_SET_DTR_MASK << 8))
#define | SIO_SET_RTS_MASK 0x2
#define | SIO_SET_RTS_HIGH ( 2 | ( SIO_SET_RTS_MASK << 8 ))
#define | SIO_SET_RTS_LOW ( 0 | ( SIO_SET_RTS_MASK << 8 ))
#define | SIO_RTS_CTS_HS (0x1 << 8)
#define | FTDI_URB_USERCONTEXT_COOKIE ((void *)0x1)
#define | DEPRECATED(func) func
#define | FT1284_CLK_IDLE_STATE 0x01
#define | FT1284_DATA_LSB 0x02 /* DS_FT232H 1.3 amd ftd2xx.h 1.0.4 disagree here*/
#define | FT1284_FLOW_CONTROL 0x04
#define | POWER_SAVE_DISABLE_H 0x80
#define | USE_SERIAL_NUM 0x08
#define | INVERT_TXD 0x01
#define | INVERT_RXD 0x02
#define | INVERT_RTS 0x04
#define | INVERT_CTS 0x08
#define | INVERT_DTR 0x10
#define | INVERT_DSR 0x20
#define | INVERT_DCD 0x40
#define | INVERT_RI 0x80
#define | CHANNEL_IS_UART 0x0
#define | CHANNEL_IS_FIFO 0x1
#define | CHANNEL_IS_OPTO 0x2
#define | CHANNEL_IS_CPU 0x4
#define | CHANNEL_IS_FT1284 0x8
#define | CHANNEL_IS_RS485 0x10
#define | DRIVE_4MA 0
#define | DRIVE_8MA 1
#define | DRIVE_12MA 2
#define | DRIVE_16MA 3
#define | SLOW_SLEW 4
#define | IS_SCHMITT 8
#define | DRIVER_VCP 0x08
#define | DRIVER_VCPH 0x10 /* FT232H has moved the VCP bit */
#define | USE_USB_VERSION_BIT 0x10
#define | SUSPEND_DBUS7_BIT 0x80
#define | HIGH_CURRENT_DRIVE 0x10
#define | HIGH_CURRENT_DRIVE_R 0x04

## Typedefs
typedef int( | FTDIStreamCallback )(uint8_t *buffer, int length, FTDIProgressInfo *progress, void *userdata)

## Enumerations
enum | ftdi_chip_type { TYPE_AM =0, TYPE_BM =1, TYPE_2232C =2, TYPE_R =3, TYPE_2232H =4, TYPE_4232H =5, TYPE_232H =6 }
enum | ftdi_parity_type { NONE =0, ODD =1, EVEN =2, MARK =3, SPACE =4 }
enum | ftdi_stopbits_type { STOP_BIT_1 =0, STOP_BIT_15 =1, STOP_BIT_2 =2 }
enum | ftdi_bits_type { BITS_7 =7, BITS_8 =8 }
enum | ftdi_break_type { BREAK_OFF =0, BREAK_ON =1 }
enum | ftdi_mpsse_mode { BITMODE_RESET = 0x00, BITMODE_BITBANG = 0x01, BITMODE_MPSSE = 0x02, BITMODE_SYNCBB = 0x04, BITMODE_MCU = 0x08, BITMODE_OPTO = 0x10, BITMODE_CBUS = 0x20, BITMODE_SYNCFF = 0x40, BITMODE_FT1284 = 0x80 }
enum | ftdi_interface { INTERFACE_ANY = 0, INTERFACE_A = 1, INTERFACE_B = 2, INTERFACE_C = 3, INTERFACE_D = 4 }
enum | ftdi_module_detach_mode { AUTO_DETACH_SIO_MODULE = 0, DONT_DETACH_SIO_MODULE = 1 }
enum | ftdi_eeprom_value { VENDOR_ID = 0, PRODUCT_ID = 1, SELF_POWERED = 2, REMOTE_WAKEUP = 3, IS_NOT_PNP = 4, SUSPEND_DBUS7 = 5, IN_IS_ISOCHRONOUS = 6, OUT_IS_ISOCHRONOUS = 7, SUSPEND_PULL_DOWNS = 8, USE_SERIAL = 9, USB_VERSION = 10, USE_USB_VERSION = 11, MAX_POWER = 12, CHANNEL_A_TYPE = 13, CHANNEL_B_TYPE = 14, CHANNEL_A_DRIVER = 15, CHANNEL_B_DRIVER = 16, CBUS_FUNCTION_0 = 17, CBUS_FUNCTION_1 = 18, CBUS_FUNCTION_2 = 19, CBUS_FUNCTION_3 = 20, CBUS_FUNCTION_4 = 21, CBUS_FUNCTION_5 = 22, CBUS_FUNCTION_6 = 23, CBUS_FUNCTION_7 = 24, CBUS_FUNCTION_8 = 25, CBUS_FUNCTION_9 = 26, HIGH_CURRENT = 27, HIGH_CURRENT_A = 28, HIGH_CURRENT_B = 29, INVERT = 30, GROUP0_DRIVE = 31, GROUP0_SCHMITT = 32, GROUP0_SLEW = 33, GROUP1_DRIVE = 34, GROUP1_SCHMITT = 35, GROUP1_SLEW = 36, GROUP2_DRIVE = 37, GROUP2_SCHMITT = 38, GROUP2_SLEW = 39, GROUP3_DRIVE = 40, GROUP3_SCHMITT = 41, GROUP3_SLEW = 42, CHIP_SIZE = 43, CHIP_TYPE = 44, POWER_SAVE = 45, CLOCK_POLARITY = 46, DATA_ORDER = 47, FLOW_CONTROL = 48, CHANNEL_C_DRIVER = 49, CHANNEL_D_DRIVER = 50, CHANNEL_A_RS485 = 51, CHANNEL_B_RS485 = 52, CHANNEL_C_RS485 = 53, CHANNEL_D_RS485 = 54 }
enum | ftdi_cbus_func { CBUS_TXDEN = 0, CBUS_PWREN = 1, CBUS_RXLED = 2, CBUS_TXLED = 3, CBUS_TXRXLED = 4, CBUS_SLEEP = 5, CBUS_CLK48 = 6, CBUS_CLK24 = 7, CBUS_CLK12 = 8, CBUS_CLK6 = 9, CBUS_IOMODE = 0xa, CBUS_BB_WR = 0xb, CBUS_BB_RD = 0xc, CBUS_BB = 0xd }
enum | ftdi_cbush_func { CBUSH_TRISTATE = 0, CBUSH_RXLED = 1, CBUSH_TXLED = 2, CBUSH_TXRXLED = 3, CBUSH_PWREN = 4, CBUSH_SLEEP = 5, CBUSH_DRIVE_0 = 6, CBUSG_DRIVE1 = 7, CBUSH_IOMODE = 8, CBUSH_TXDEN = 9, CBUSH_CLK30 = 0xa, CBUSH_CLK15 = 0xb, CBUSH_CLK7_5 = 0xc }

## Functions
int | ftdi_init (struct ftdi_context *ftdi)
struct ftdi_context * | ftdi_new (void)
int | ftdi_set_interface (struct ftdi_context *ftdi, enum ftdi_interface interface)
void | ftdi_deinit (struct ftdi_context *ftdi)
void | ftdi_free (struct ftdi_context *ftdi)
void | ftdi_set_usbdev (struct ftdi_context *ftdi, struct libusb_device_handle *usbdev)
struct ftdi_version_info | ftdi_get_library_version ()
| Get libftdi library version.
int | ftdi_usb_find_all (struct ftdi_context *ftdi, struct ftdi_device_list **devlist, int vendor, int product)
void | ftdi_list_free (struct ftdi_device_list **devlist)
void | ftdi_list_free2 (struct ftdi_device_list *devlist)
int | ftdi_usb_get_strings (struct ftdi_context *ftdi, struct libusb_device *dev, char *manufacturer, int mnf_len, char *description, int desc_len, char *serial, int serial_len)
int | ftdi_usb_open (struct ftdi_context *ftdi, int vendor, int product)
int | ftdi_usb_open_desc (struct ftdi_context *ftdi, int vendor, int product, const char *description, const char *serial)
int | ftdi_usb_open_desc_index (struct ftdi_context *ftdi, int vendor, int product, const char *description, const char *serial, unsigned int index)
int | ftdi_usb_open_dev (struct ftdi_context *ftdi, struct libusb_device *dev)
int | ftdi_usb_open_string (struct ftdi_context *ftdi, const char *description)
int | ftdi_usb_close (struct ftdi_context *ftdi)
int | ftdi_usb_reset (struct ftdi_context *ftdi)
int | ftdi_usb_purge_rx_buffer (struct ftdi_context *ftdi)
int | ftdi_usb_purge_tx_buffer (struct ftdi_context *ftdi)
int | ftdi_usb_purge_buffers (struct ftdi_context *ftdi)
int | ftdi_set_baudrate (struct ftdi_context *ftdi, int baudrate)
int | ftdi_set_line_property (struct ftdi_context *ftdi, enum ftdi_bits_type bits, enum ftdi_stopbits_type sbit, enum ftdi_parity_type parity)
int | ftdi_set_line_property2 (struct ftdi_context *ftdi, enum ftdi_bits_type bits, enum ftdi_stopbits_type sbit, enum ftdi_parity_type parity, enum ftdi_break_type break_type)
int | ftdi_read_data (struct ftdi_context *ftdi, unsigned char *buf, int size)
int | ftdi_read_data_set_chunksize (struct ftdi_context *ftdi, unsigned int chunksize)
int | ftdi_read_data_get_chunksize (struct ftdi_context *ftdi, unsigned int *chunksize)
int | ftdi_write_data (struct ftdi_context *ftdi, unsigned char *buf, int size)
int | ftdi_write_data_set_chunksize (struct ftdi_context *ftdi, unsigned int chunksize)
int | ftdi_write_data_get_chunksize (struct ftdi_context *ftdi, unsigned int *chunksize)
int | ftdi_readstream (struct ftdi_context *ftdi, FTDIStreamCallback *callback, void *userdata, int packetsPerTransfer, int numTransfers)
struct ftdi_transfer_control * | ftdi_write_data_submit (struct ftdi_context *ftdi, unsigned char *buf, int size)
struct ftdi_transfer_control * | ftdi_read_data_submit (struct ftdi_context *ftdi, unsigned char *buf, int size)
int | ftdi_transfer_data_done (struct ftdi_transfer_control *tc)
int | ftdi_set_bitmode (struct ftdi_context *ftdi, unsigned char bitmask, unsigned char mode)
int | ftdi_disable_bitbang (struct ftdi_context *ftdi)
int | ftdi_read_pins (struct ftdi_context *ftdi, unsigned char *pins)
int | ftdi_set_latency_timer (struct ftdi_context *ftdi, unsigned char latency)
int | ftdi_get_latency_timer (struct ftdi_context *ftdi, unsigned char *latency)
int | ftdi_poll_modem_status (struct ftdi_context *ftdi, unsigned short *status)
int | ftdi_setflowctrl (struct ftdi_context *ftdi, int flowctrl)
int | ftdi_setdtr_rts (struct ftdi_context *ftdi, int dtr, int rts)
int | ftdi_setdtr (struct ftdi_context *ftdi, int state)
int | ftdi_setrts (struct ftdi_context *ftdi, int state)
int | ftdi_set_event_char (struct ftdi_context *ftdi, unsigned char eventch, unsigned char enable)
int | ftdi_set_error_char (struct ftdi_context *ftdi, unsigned char errorch, unsigned char enable)
int | ftdi_eeprom_initdefaults (struct ftdi_context *ftdi, char *manufacturer, char *product, char *serial)
int | ftdi_eeprom_build (struct ftdi_context *ftdi)
int | ftdi_eeprom_decode (struct ftdi_context *ftdi, int verbose)
int | ftdi_get_eeprom_value (struct ftdi_context *ftdi, enum ftdi_eeprom_value value_name, int *value)
int | ftdi_set_eeprom_value (struct ftdi_context *ftdi, enum ftdi_eeprom_value value_name, int value)
int | ftdi_get_eeprom_buf (struct ftdi_context *ftdi, unsigned char *buf, int size)
int | ftdi_set_eeprom_buf (struct ftdi_context *ftdi, const unsigned char *buf, int size)
int | ftdi_read_eeprom (struct ftdi_context *ftdi)
int | ftdi_read_chipid (struct ftdi_context *ftdi, unsigned int *chipid)
int | ftdi_write_eeprom (struct ftdi_context *ftdi)
int | ftdi_erase_eeprom (struct ftdi_context *ftdi)
int | ftdi_read_eeprom_location (struct ftdi_context *ftdi, int eeprom_addr, unsigned short *eeprom_val)
int | ftdi_write_eeprom_location (struct ftdi_context *ftdi, int eeprom_addr, unsigned short eeprom_val)
char * | ftdi_get_error_string (struct ftdi_context *ftdi)

## Macro Definition Documentation

#define MPSSE_WRITE_NEG 0x01 /* Write TDI/DO on negative TCK/SK edge*/

Definition at line 67 of file ftdi.h.

#define MPSSE_BITMODE 0x02 /* Write bits, not bytes */

Definition at line 68 of file ftdi.h.

#define MPSSE_READ_NEG 0x04 /* Sample TDO/DI on negative TCK/SK edge */

Definition at line 69 of file ftdi.h.

#define MPSSE_LSB 0x08 /* LSB first */

Definition at line 70 of file ftdi.h.

#define MPSSE_DO_WRITE 0x10 /* Write TDI/DO */

Definition at line 71 of file ftdi.h.

#define MPSSE_DO_READ 0x20 /* Read TDO/DI */

Definition at line 72 of file ftdi.h.

#define MPSSE_WRITE_TMS 0x40 /* Write TMS/CS */

Definition at line 73 of file ftdi.h.

#define SET_BITS_LOW 0x80

Definition at line 76 of file ftdi.h.

#define SET_BITS_HIGH 0x82

Definition at line 79 of file ftdi.h.

#define GET_BITS_LOW 0x81

Definition at line 82 of file ftdi.h.

#define GET_BITS_HIGH 0x83

Definition at line 83 of file ftdi.h.

#define LOOPBACK_START 0x84

Definition at line 84 of file ftdi.h.

#define LOOPBACK_END 0x85

Definition at line 85 of file ftdi.h.

#define TCK_DIVISOR 0x86

Definition at line 86 of file ftdi.h.

#define DIS_DIV_5 0x8a

Definition at line 88 of file ftdi.h.

#define EN_DIV_5 0x8b

Definition at line 89 of file ftdi.h.

#define EN_3_PHASE 0x8c

Definition at line 90 of file ftdi.h.

#define DIS_3_PHASE 0x8d

Definition at line 91 of file ftdi.h.

#define CLK_BITS 0x8e

Definition at line 92 of file ftdi.h.

#define CLK_BYTES 0x8f

Definition at line 93 of file ftdi.h.

#define CLK_WAIT_HIGH 0x94

Definition at line 94 of file ftdi.h.

#define CLK_WAIT_LOW 0x95

Definition at line 95 of file ftdi.h.

#define EN_ADAPTIVE 0x96

Definition at line 96 of file ftdi.h.

#define DIS_ADAPTIVE 0x97

Definition at line 97 of file ftdi.h.

#define CLK_BYTES_OR_HIGH 0x9c

Definition at line 98 of file ftdi.h.

#define CLK_BYTES_OR_LOW 0x0d

Definition at line 99 of file ftdi.h.

#define DRIVE_OPEN_COLLECTOR 0x9e

Definition at line 101 of file ftdi.h.

#define DIV_VALUE | ( |  | rate | ) | (rate > 6000000)?0:((6000000/rate -1) > 0xffff)? 0xffff: (6000000/rate -1)

Definition at line 104 of file ftdi.h.

#define SEND_IMMEDIATE 0x87

Definition at line 107 of file ftdi.h.

#define WAIT_ON_HIGH 0x88

Definition at line 108 of file ftdi.h.

#define WAIT_ON_LOW 0x89

Definition at line 109 of file ftdi.h.

#define READ_SHORT 0x90

Definition at line 112 of file ftdi.h.

#define READ_EXTENDED 0x91

Definition at line 114 of file ftdi.h.

#define WRITE_SHORT 0x92

Definition at line 117 of file ftdi.h.

#define WRITE_EXTENDED 0x93

Definition at line 119 of file ftdi.h.

#define SIO_RESET 0 /* Reset the port */

Definition at line 124 of file ftdi.h.

#define SIO_MODEM_CTRL 1 /* Set the modem control register */

Definition at line 125 of file ftdi.h.

#define SIO_SET_FLOW_CTRL 2 /* Set flow control register */

Definition at line 126 of file ftdi.h.

#define SIO_SET_BAUD_RATE 3 /* Set baud rate */

Definition at line 127 of file ftdi.h.

#define SIO_SET_DATA 4 /* Set the data characteristics of the port */

Definition at line 128 of file ftdi.h.

#define FTDI_DEVICE_OUT_REQTYPE (LIBUSB_REQUEST_TYPE_VENDOR | LIBUSB_RECIPIENT_DEVICE | LIBUSB_ENDPOINT_OUT)

Definition at line 130 of file ftdi.h.

Referenced by ftdi_disable_bitbang(), ftdi_erase_eeprom(), ftdi_set_baudrate(), ftdi_set_bitmode(), ftdi_set_error_char(), ftdi_set_event_char(), ftdi_set_latency_timer(), ftdi_set_line_property2(), ftdi_setdtr(), ftdi_setdtr_rts(), ftdi_setflowctrl(), ftdi_setrts(), ftdi_usb_purge_rx_buffer(), ftdi_usb_purge_tx_buffer(), ftdi_usb_reset(), ftdi_write_eeprom(), and ftdi_write_eeprom_location().

#define FTDI_DEVICE_IN_REQTYPE (LIBUSB_REQUEST_TYPE_VENDOR | LIBUSB_RECIPIENT_DEVICE | LIBUSB_ENDPOINT_IN)

Definition at line 131 of file ftdi.h.

Referenced by ftdi_get_latency_timer(), ftdi_poll_modem_status(), ftdi_read_chipid(), ftdi_read_eeprom(), ftdi_read_eeprom_location(), and ftdi_read_pins().

#define SIO_RESET_REQUEST SIO_RESET

Definition at line 134 of file ftdi.h.

Referenced by ftdi_usb_purge_rx_buffer(), ftdi_usb_purge_tx_buffer(), and ftdi_usb_reset().

#define SIO_SET_BAUDRATE_REQUEST SIO_SET_BAUD_RATE

Definition at line 135 of file ftdi.h.

Referenced by ftdi_set_baudrate().

#define SIO_SET_DATA_REQUEST SIO_SET_DATA

Definition at line 136 of file ftdi.h.

Referenced by ftdi_set_line_property2().

#define SIO_SET_FLOW_CTRL_REQUEST SIO_SET_FLOW_CTRL

Definition at line 137 of file ftdi.h.

Referenced by ftdi_setflowctrl().

#define SIO_SET_MODEM_CTRL_REQUEST SIO_MODEM_CTRL

Definition at line 138 of file ftdi.h.

Referenced by ftdi_setdtr(), ftdi_setdtr_rts(), and ftdi_setrts().

#define SIO_POLL_MODEM_STATUS_REQUEST 0x05

Definition at line 139 of file ftdi.h.

Referenced by ftdi_poll_modem_status().

#define SIO_SET_EVENT_CHAR_REQUEST 0x06

Definition at line 140 of file ftdi.h.

Referenced by ftdi_set_event_char().

#define SIO_SET_ERROR_CHAR_REQUEST 0x07

Definition at line 141 of file ftdi.h.

Referenced by ftdi_set_error_char().

#define SIO_SET_LATENCY_TIMER_REQUEST 0x09

Definition at line 142 of file ftdi.h.

Referenced by ftdi_set_latency_timer().

#define SIO_GET_LATENCY_TIMER_REQUEST 0x0A

Definition at line 143 of file ftdi.h.

Referenced by ftdi_get_latency_timer().

#define SIO_SET_BITMODE_REQUEST 0x0B

Definition at line 144 of file ftdi.h.

Referenced by ftdi_disable_bitbang(), and ftdi_set_bitmode().

#define SIO_READ_PINS_REQUEST 0x0C

Definition at line 145 of file ftdi.h.

Referenced by ftdi_read_pins().

#define SIO_READ_EEPROM_REQUEST 0x90

Definition at line 146 of file ftdi.h.

Referenced by ftdi_read_chipid(), ftdi_read_eeprom(), and ftdi_read_eeprom_location().

#define SIO_WRITE_EEPROM_REQUEST 0x91

Definition at line 147 of file ftdi.h.

Referenced by ftdi_erase_eeprom(), ftdi_write_eeprom(), and ftdi_write_eeprom_location().

#define SIO_ERASE_EEPROM_REQUEST 0x92

Definition at line 148 of file ftdi.h.

Referenced by ftdi_erase_eeprom().

#define SIO_RESET_SIO 0

Definition at line 151 of file ftdi.h.

Referenced by ftdi_usb_reset().

#define SIO_RESET_PURGE_RX 1

Definition at line 152 of file ftdi.h.

Referenced by ftdi_usb_purge_rx_buffer().

#define SIO_RESET_PURGE_TX 2

Definition at line 153 of file ftdi.h.

Referenced by ftdi_usb_purge_tx_buffer().

#define SIO_DISABLE_FLOW_CTRL 0x0

Definition at line 155 of file ftdi.h.

#define SIO_RTS_CTS_HS (0x1 << 8)

Definition at line 167 of file ftdi.h.

#define SIO_DTR_DSR_HS (0x2 << 8)

Definition at line 157 of file ftdi.h.

#define SIO_XON_XOFF_HS (0x4 << 8)

Definition at line 158 of file ftdi.h.

#define SIO_SET_DTR_MASK 0x1

Definition at line 160 of file ftdi.h.

#define SIO_SET_DTR_HIGH ( 1 | ( SIO_SET_DTR_MASK << 8))

Definition at line 161 of file ftdi.h.

Referenced by ftdi_setdtr(), and ftdi_setdtr_rts().

#define SIO_SET_DTR_LOW ( 0 | ( SIO_SET_DTR_MASK << 8))

Definition at line 162 of file ftdi.h.

Referenced by ftdi_setdtr(), and ftdi_setdtr_rts().

#define SIO_SET_RTS_MASK 0x2

Definition at line 163 of file ftdi.h.

#define SIO_SET_RTS_HIGH ( 2 | ( SIO_SET_RTS_MASK << 8 ))

Definition at line 164 of file ftdi.h.

Referenced by ftdi_setdtr_rts(), and ftdi_setrts().

#define SIO_SET_RTS_LOW ( 0 | ( SIO_SET_RTS_MASK << 8 ))

Definition at line 165 of file ftdi.h.

Referenced by ftdi_setdtr_rts(), and ftdi_setrts().

#define SIO_RTS_CTS_HS (0x1 << 8)

Definition at line 167 of file ftdi.h.

#define FTDI_URB_USERCONTEXT_COOKIE ((void *)0x1)

Definition at line 171 of file ftdi.h.

#define DEPRECATED | ( |  | func | ) | func

Definition at line 179 of file ftdi.h.

#define FT1284_CLK_IDLE_STATE 0x01

Definition at line 324 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define FT1284_DATA_LSB 0x02 /* DS_FT232H 1.3 amd ftd2xx.h 1.0.4 disagree here*/

Definition at line 325 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define FT1284_FLOW_CONTROL 0x04

Definition at line 326 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define POWER_SAVE_DISABLE_H 0x80

Definition at line 327 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define USE_SERIAL_NUM 0x08

Definition at line 329 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define INVERT_TXD 0x01

Invert TXD#

Definition at line 341 of file ftdi.h.

#define INVERT_RXD 0x02

Invert RXD#

Definition at line 343 of file ftdi.h.

#define INVERT_RTS 0x04

Invert RTS#

Definition at line 345 of file ftdi.h.

#define INVERT_CTS 0x08

Invert CTS#

Definition at line 347 of file ftdi.h.

#define INVERT_DTR 0x10

Invert DTR#

Definition at line 349 of file ftdi.h.

#define INVERT_DSR 0x20

Invert DSR#

Definition at line 351 of file ftdi.h.

#define INVERT_DCD 0x40

Invert DCD#

Definition at line 353 of file ftdi.h.

#define INVERT_RI 0x80

Invert RI#

Definition at line 355 of file ftdi.h.

#define CHANNEL_IS_UART 0x0

Interface Mode.

Definition at line 358 of file ftdi.h.

#define CHANNEL_IS_FIFO 0x1

Definition at line 359 of file ftdi.h.

#define CHANNEL_IS_OPTO 0x2

Definition at line 360 of file ftdi.h.

#define CHANNEL_IS_CPU 0x4

Definition at line 361 of file ftdi.h.

#define CHANNEL_IS_FT1284 0x8

Definition at line 362 of file ftdi.h.

#define CHANNEL_IS_RS485 0x10

Definition at line 364 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define DRIVE_4MA 0

Definition at line 366 of file ftdi.h.

#define DRIVE_8MA 1

Definition at line 367 of file ftdi.h.

#define DRIVE_12MA 2

Definition at line 368 of file ftdi.h.

#define DRIVE_16MA 3

Definition at line 369 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define SLOW_SLEW 4

Definition at line 370 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define IS_SCHMITT 8

Definition at line 371 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define DRIVER_VCP 0x08

Driver Type.

Definition at line 374 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define DRIVER_VCPH 0x10 /* FT232H has moved the VCP bit */

Definition at line 375 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define USE_USB_VERSION_BIT 0x10

Definition at line 377 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define SUSPEND_DBUS7_BIT 0x80

Definition at line 379 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define HIGH_CURRENT_DRIVE 0x10

High current drive.

Definition at line 382 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

#define HIGH_CURRENT_DRIVE_R 0x04

Definition at line 383 of file ftdi.h.

Referenced by ftdi_eeprom_build(), and ftdi_eeprom_decode().

## Typedef Documentation

typedef int( FTDIStreamCallback)(uint8_t *buffer, int length, FTDIProgressInfo *progress, void *userdata)

Definition at line 404 of file ftdi.h.

## Enumeration Type Documentation

enum ftdi_chip_type

FTDI chip type

Enumerator
TYPE_AM |
TYPE_BM |
TYPE_2232C |
TYPE_R |
TYPE_2232H |
TYPE_4232H |
TYPE_232H |

Definition at line 24 of file ftdi.h.

enum ftdi_parity_type

Parity mode for ftdi_set_line_property()

Enumerator
NONE |
ODD |
EVEN |
MARK |
SPACE |

Definition at line 26 of file ftdi.h.

enum ftdi_stopbits_type

Number of stop bits for ftdi_set_line_property()

Enumerator
STOP_BIT_1 |
STOP_BIT_15 |
STOP_BIT_2 |

Definition at line 28 of file ftdi.h.

enum ftdi_bits_type

Number of bits for ftdi_set_line_property()

Enumerator
BITS_7 |
BITS_8 |

Definition at line 30 of file ftdi.h.

enum ftdi_break_type

Break type for ftdi_set_line_property2()

Enumerator
BREAK_OFF |
BREAK_ON |

Definition at line 32 of file ftdi.h.

enum ftdi_mpsse_mode

MPSSE bitbang modes

Enumerator
BITMODE_RESET | switch off bitbang mode, back to regular serial/FIFO
BITMODE_BITBANG | classical asynchronous bitbang mode, introduced with B-type chips
BITMODE_MPSSE | MPSSE mode, available on 2232x chips
BITMODE_SYNCBB | synchronous bitbang mode, available on 2232x and R-type chips
BITMODE_MCU | MCU Host Bus Emulation mode, available on 2232x chips
BITMODE_OPTO | Fast Opto-Isolated Serial Interface Mode, available on 2232x chips
BITMODE_CBUS | Bitbang on CBUS pins of R-type chips, configure in EEPROM before
BITMODE_SYNCFF | Single Channel Synchronous FIFO mode, available on 2232H chips
BITMODE_FT1284 | FT1284 mode, available on 232H chips

Definition at line 35 of file ftdi.h.

enum ftdi_interface

Port interface for chips with multiple interfaces

Enumerator
INTERFACE_ANY |
INTERFACE_A |
INTERFACE_B |
INTERFACE_C |
INTERFACE_D |

Definition at line 50 of file ftdi.h.

enum ftdi_module_detach_mode

Automatic loading / unloading of kernel modules

Enumerator
AUTO_DETACH_SIO_MODULE |
DONT_DETACH_SIO_MODULE |

Definition at line 60 of file ftdi.h.

enum ftdi_eeprom_value

List all handled EEPROM values. Append future new values only at the end to provide API/ABI stability

Enumerator
VENDOR_ID |
PRODUCT_ID |
SELF_POWERED |
REMOTE_WAKEUP |
IS_NOT_PNP |
SUSPEND_DBUS7 |
IN_IS_ISOCHRONOUS |
OUT_IS_ISOCHRONOUS |
SUSPEND_PULL_DOWNS |
USE_SERIAL |
USB_VERSION |
USE_USB_VERSION |
MAX_POWER |
CHANNEL_A_TYPE |
CHANNEL_B_TYPE |
CHANNEL_A_DRIVER |
CHANNEL_B_DRIVER |
CBUS_FUNCTION_0 |
CBUS_FUNCTION_1 |
CBUS_FUNCTION_2 |
CBUS_FUNCTION_3 |
CBUS_FUNCTION_4 |
CBUS_FUNCTION_5 |
CBUS_FUNCTION_6 |
CBUS_FUNCTION_7 |
CBUS_FUNCTION_8 |
CBUS_FUNCTION_9 |
HIGH_CURRENT |
HIGH_CURRENT_A |
HIGH_CURRENT_B |
INVERT |
GROUP0_DRIVE |
GROUP0_SCHMITT |
GROUP0_SLEW |
GROUP1_DRIVE |
GROUP1_SCHMITT |
GROUP1_SLEW |
GROUP2_DRIVE |
GROUP2_SCHMITT |
GROUP2_SLEW |
GROUP3_DRIVE |
GROUP3_SCHMITT |
GROUP3_SLEW |
CHIP_SIZE |
CHIP_TYPE |
POWER_SAVE |
CLOCK_POLARITY |
DATA_ORDER |
FLOW_CONTROL |
CHANNEL_C_DRIVER |
CHANNEL_D_DRIVER |
CHANNEL_A_RS485 |
CHANNEL_B_RS485 |
CHANNEL_C_RS485 |
CHANNEL_D_RS485 |

Definition at line 255 of file ftdi.h.

enum ftdi_cbus_func

Enumerator
CBUS_TXDEN |
CBUS_PWREN |
CBUS_RXLED |
CBUS_TXLED |
CBUS_TXRXLED |
CBUS_SLEEP |
CBUS_CLK48 |
CBUS_CLK24 |
CBUS_CLK12 |
CBUS_CLK6 |
CBUS_IOMODE |
CBUS_BB_WR |
CBUS_BB_RD |
CBUS_BB |

Definition at line 330 of file ftdi.h.

enum ftdi_cbush_func

Enumerator
CBUSH_TRISTATE |
CBUSH_RXLED |
CBUSH_TXLED |
CBUSH_TXRXLED |
CBUSH_PWREN |
CBUSH_SLEEP |
CBUSH_DRIVE_0 |
CBUSG_DRIVE1 |
CBUSH_IOMODE |
CBUSH_TXDEN |
CBUSH_CLK30 |
CBUSH_CLK15 |
CBUSH_CLK7_5 |

Definition at line 335 of file ftdi.h.

## Function Documentation

int ftdi_readstream | ( | struct ftdi_context * | ftdi,
|  | FTDIStreamCallback * | callback,
|  | void * | userdata,
|  | int | packetsPerTransfer,
|  | int | numTransfers
| ) |  |

Streaming reading of data from the device

Use asynchronous transfers in libusb-1.0 for high-performance streaming of data from a device interface back to the PC. This function continuously transfers data until either an error occurs or the callback returns a nonzero value. This function returns a libusb error code or the callback's return value.

For every contiguous block of received data, the callback will be invoked.

Parameters

  ftdi | pointer to ftdi_context
  callback | to user supplied function for one block of data
  userdata |
  packetsPerTransfer | number of packets per transfer
  numTransfers | Number of transfers per callback

Definition at line 147 of file ftdi_stream.c.

References FTDIStreamState::activity, BITMODE_RESET, BITMODE_SYNCFF, FTDIStreamState::callback, FTDIProgressInfo::current, FTDIProgressInfo::currentRate, FTDIProgressInfo::first, ftdi_get_error_string(), ftdi_set_bitmode(), ftdi_usb_purge_buffers(), ftdi_context::max_packet_size, ftdi_context::out_ep, FTDIProgressInfo::prev, FTDIStreamState::progress, FTDIStreamState::result, size_and_time::time, size_and_time::totalBytes, FTDIProgressInfo::totalRate, FTDIProgressInfo::totalTime, ftdi_context::type, TYPE_2232H, TYPE_232H, ftdi_context::usb_ctx, ftdi_context::usb_dev, ftdi_context::usb_read_timeout, and FTDIStreamState::userdata.