1. Right Click where it says EPOS 2 under the COM port and select “Connect”. This will take a few seconds and you will see the software talking to the motor controller
2. Select the tab that says “I/O monitor”, this is where you will turn the limit switches on.
a. The Positive (or lower limit switch) is Digital 1
b. The Negative (or upper limit switch) is Digital input 2
c. Enable each digital input under the column “Exec Mask”, using the pull down menu.
3. Select the tab that says Velocity Mode
a. Press “Activate Velocity Mode in the upper left
b. Set the velocity to 500 rpm under “Setting Value” Remember positive tilts the camera down and negative tilts the camera up
c. Then in low left hand corner clicke on “disabled” to enable the drive
d. Before you start moving know that you can stop the motion by pressing “Quickstop”
e. To move the motor click on “Apply the setting value”
f. You may want to arrange your windows on the laptop so you can see the liveview and the motor controller software at the same time.
g. Stop when you want by pressing quickstop.
h. To start again you will need to press “Quickstop” again and then press apply setting value.
i. If you trigger a limit switch you need to go into the lower status window and right click on the error and select “Clear All Errors” 
j. [bookmark: _GoBack]When you are happy with the position disable the motor and then close the EPOS software.
