Multi-Spectral LED Board Test Plan


Initially populate three pcbs
	2 with common ground plane
	1 with split ground plane

Compare PWM vs analog dimming.
	Does the PWM signal influence the noise level?
	Measure the extinction ratio difference.

Ripple current on LED drive signals.
	Output circuit L’s and C’s (refer to excel file)
	Can parallel caps for greater capacitance
	Monitor with Denis’ photodiode

Acoustic noise generated by electrical components.
	Test in Kelly’s lab
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