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Camera
Camera Vendor: SubC	model: 
Serial #:
Internal camera module manufacturer: Sony FCB-ER8300?
Video interface
Uplink media:	SM fiber	Uplink protocol: Fiber to HDMI
Control interface
Link media:	232/485		Link protocol: 
Camera control interface
Camera settings control evaluation:

Camera lens control interface
Camera lens settings control evaluation.
Quality of control box:
Camera lens zoom control smoothness:
Camera lens focus control precision:
		
1. Interface design and ease of installation.
      a. Video uplink quality and properties.
      b. Control downlink quality and properties.
3. User controls and settings.
      a. Smoothness and precision of zoom and focus.
      b. Ability to adjust camera settings.
      c. Quality and ease of use of control box.
4. Test tank measurement of field of view at 0.5, 1 and 2 meters.
[bookmark: _GoBack]5. Test tank resolution and distortion evaluation. Note that camera has a flat plate front adapter. (not a dome).
6. Test tank depth of field evaluation at specified wide open lens iris setting at 0.5 and 1 meters.
7. Test tank color reproduction evaluation.
8. Lab test of light sensitivity.
9. Price and availability.
10. Reputation of the manufacturer and record of customer service on repairs.

[image: ]
image1.emf
Date:

Recording #

Distance 

of Target 

from 

Dome

Focus 

Setting

Iris 

Setting

Zoom 

Setting

Shutter 

Setting

20180621T141643

1.02 

meter

? 100% wide ?

20180621T142004

1.02 

meter

? 100% wide ?

UHD Camera Evaluation Clip Descriptions


