Procedure for installing firmware updates for the HDC-P50 camera.
1. Verify the current firmware version currently in the camera by accessing the camera menu diagnostics page. Read the service manual procedure on firmware updates.
2. Contact Bill Peters, William.Peters@sony.com, or other tech support at Sony to obtain the current firmware release. Note that you may have to go through several sequential upgrades if the camera is very out of date.
3. [bookmark: _GoBack]The USB drive used is important! I have only been able to get an old Sony “data vault” 2 GB USB stick to work. If the camera is powered up with the USB stick in place, the monitor display menu will briefly show the USB mount status on power up. If the USB drive fails to mount you need to use another drive.
4. The project folder location where updates are stored: \\atlas\ProjectLibrary\902001_4K_ROVCameraDevelopment\EngineeringDesignDocuments\4K_SonyHDC-P50_Data\4K_LicenseKeys&FirmwareUpdates\FirmwareUpdates
5. The update firmware directory will have at least three files, the hdcp50_os.pkg (operating system), hdcp50_app.pkg (application) and the hdcp50_updater.pkg (updater).
6. Follow the instructions in the service manual to perform the update with the following additional notes:
a. Note that the firmware updates all have the same filenames, so you must copy them into the update folder tree and perform an update one version at a time.
b. ALWAYS update the OS firmware first! Not doing this will brick the camera (if this happens see “forced version update in the service manual”).
c. Then update the application and updater firmware.
d. Verify the firmware updates after a camera power cycle.
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