100221507-04-A 4K Camera Lapbox ECO List for REV. A PCB

09JUL21 – mrc
[bookmark: _GoBack]ECO #1: Reconfigure U16 A/D for proper input connections.
A. Remove R8 and R13.
B. Connect blue wire from R13 PAD on U16 side to U15A PIN 1.
C. Connect blue wire from R8 PAD on U16 side to U15B pins 6 or 7. Note 6&7 are connected together on PCB.
ECO #2: Change analog input resistor values.
A. Replace R14 with 100 Ohm resistor.
B. Replace R45 with 35.70 K Ohm resistor.
C. Replace R22 with 30.10 K Ohm resistor.
D. Replace R21 with 26.7 K Ohm resistor.
E. Replace R19 with 100 Ohm resistor.
F. Replace R44 with 35.70 K Ohm resistor.
G. Replace R28 with 30.10 K Ohm resistor.
H. Replace R29 with 26.7 K Ohm resistor.
ECO #3: Take out resistors.
A. Replace R47 and R27 with either 0 Ohm resistor or bridge pads.
ECO #4: Replace resistors.
A. Replace R33 and R46 with 232 Ohm resistors.
ECO #5: Change COM power source to 24V on LED low side drivers.
A. Raise PIN 9 lead from PAD on U3 and U2.
B. Blue wire U3 and U2 PIN 9 to positive (+) side of C19 (24V source).
