(footprint "1x4_050_cutout" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "1x4_2mm_cutout" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_rect (start 4.826 -1.512) (end -4.826 1.512) (layer "Edge.Cuts") (width 0.12) (fill none))
)
