(footprint "ADS4130-8_BGA" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.3 unlocked) (layer "F.SilkS"))
  (fp_text value "ADS4130-8_BGA" (at 0.1 0.1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
  (pad "A1" smd circle (at -0.8 -1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A2" smd circle (at -0.4 -1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A3" smd circle (at 0 -1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A4" smd circle (at 0.4 -1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A5" smd circle (at 0.8 -1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B1" smd circle (at -0.8 -0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B2" smd circle (at -0.4 -0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B3" smd circle (at 0 -0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B4" smd circle (at 0.4 -0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B5" smd circle (at 0.8 -0.8 90) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "C1" smd circle (at -0.8 -0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "C2" smd circle (at -0.4 -0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "C3" smd circle (at 0 -0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "C4" smd circle (at 0.4 -0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "C5" smd circle (at 0.8 -0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "D1" smd circle (at -0.8 0) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "D2" smd circle (at -0.4 0) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "D3" smd circle (at 0 0) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "D4" smd circle (at 0.4 0) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "D5" smd circle (at 0.8 0) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "E1" smd circle (at -0.8 0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "E2" smd circle (at -0.4 0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "E3" smd circle (at 0 0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "E4" smd circle (at 0.4 0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "E5" smd circle (at 0.8 0.4) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "F1" smd circle (at -0.8 0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "F2" smd circle (at -0.4 0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "F3" smd circle (at 0 0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "F4" smd circle (at 0.4 0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "F5" smd circle (at 0.8 0.8) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "G1" smd circle (at -0.8 1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "G2" smd circle (at -0.4 1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "G3" smd circle (at 0 1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "G4" smd circle (at 0.4 1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "G5" smd circle (at 0.8 1.2) (size 0.26 0.26) (layers "F.Cu" "F.Paste" "F.Mask"))
)
