(footprint "BATCOIN_2477_3039"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -9.525 -14.605 0)
		(layer "F.SilkS")
	)
	(property "Value" "BAT_3039"
		(at -7.62 13.335 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole circle
		(at -12.7 0)
		(size 2.775 2.775)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "2" thru_hole circle
		(at 12.7 0)
		(size 2.775 2.775)
		(drill 1.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "3" smd rect
		(at 0 0)
		(size 3.96 3.96)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
)
