(footprint "BAT_BRX1-2477-SM"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -12.065 -13.335 0)
		(layer "F.SilkS")
	)
	(property "Value" "BAT_BRX1-2477-SM"
		(at -5.08 19.685 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "+"
		(at 13.97 17.78 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 0 17.78 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -15.24 17.78 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -15.24 17.78 0)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at 13.97 17.78 0)
		(layer "F.Fab")
	)
	(fp_text user "-"
		(at 0 17.78 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -16 0)
		(size 5 10.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "2" smd rect
		(at 16 0)
		(size 5 10.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "3" smd rect
		(at 0 0)
		(size 5 5)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.102)
	)
)
