(footprint "BTT050_TDSO14" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0.635 -5.08 unlocked) (layer "F.SilkS"))
  (fp_text value "BTT050_TDSO14" (at 0 5.08 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0.635 -5.08 unlocked) (layer "F.Fab"))
  (pad "1" smd roundrect (at -2.9 -3.81) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "2" smd roundrect (at -2.9 -2.54) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "3" smd roundrect (at -2.9 -1.27) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "4" smd roundrect (at -2.9 0) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "5" smd roundrect (at -2.9 1.27) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "6" smd roundrect (at -2.9 2.54) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "7" smd roundrect (at -2.9 3.81) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "8" smd roundrect (at 2.9 3.81) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "9" smd roundrect (at 2.9 2.54) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "10" smd roundrect (at 2.9 1.27) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "11" smd roundrect (at 2.9 0) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "12" smd roundrect (at 2.9 -1.27) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "13" smd roundrect (at 2.9 -2.54) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "14" smd roundrect (at 2.9 -3.683) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
  (pad "15" smd roundrect (at 0 0 90) (size 6.4 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06))
)
