(footprint CONV_TPS552892RYQR (layer F.Cu) (tedit 66BBDC19)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at 0.225 -3.585 0) (layer F.SilkS))
  (fp_text value CONV_TPS552892RYQR (at 8.48 3.585 0) (layer F.Fab))
  (pad 1 smd roundrect (roundrect_rratio 0.2) (at -2.4 -0.75) (size 0.6 0.25) (layers F.Cu))
  (pad 2 smd roundrect (roundrect_rratio 0.2) (at -2.4 -0.25) (size 0.6 0.25) (layers F.Cu))
  (pad 3 smd roundrect (roundrect_rratio 0.2) (at -2.4 0.25) (size 0.6 0.25) (layers F.Cu))
  (pad 4 smd roundrect (roundrect_rratio 0.2) (at -2.4 0.75) (size 0.6 0.25) (layers F.Cu))
  (pad 5 smd roundrect (roundrect_rratio 0.2) (at -2.04 1.375) (size 0.25 0.65) (layers F.Cu))
  (pad 6 smd roundrect (roundrect_rratio 0.2) (at -1.54 1.4) (size 0.25 0.6) (layers F.Cu))
  (pad 7 smd roundrect (roundrect_rratio 0.2) (at -1.04 0.0) (size 0.25 3.4) (layers F.Cu))
  (pad 8 smd roundrect (roundrect_rratio 0.2) (at -0.54 0.0) (size 0.25 3.4) (layers F.Cu))
  (pad 10 smd roundrect (roundrect_rratio 0.2) (at 0.54 0.0) (size 0.25 3.4) (layers F.Cu))
  (pad 11 smd roundrect (roundrect_rratio 0.2) (at 1.04 0.0) (size 0.25 3.4) (layers F.Cu))
  (pad 12 smd roundrect (roundrect_rratio 0.2) (at 1.54 1.4) (size 0.25 0.6) (layers F.Cu))
  (pad 13 smd roundrect (roundrect_rratio 0.2) (at 2.04 1.375) (size 0.25 0.65) (layers F.Cu))
  (pad 14 smd roundrect (roundrect_rratio 0.2) (at 2.4 0.75) (size 0.6 0.25) (layers F.Cu))
  (pad 15 smd roundrect (roundrect_rratio 0.2) (at 2.4 0.25) (size 0.6 0.25) (layers F.Cu))
  (pad 16 smd roundrect (roundrect_rratio 0.2) (at 2.4 -0.25) (size 0.6 0.25) (layers F.Cu))
  (pad 17 smd roundrect (roundrect_rratio 0.2) (at 2.4 -0.75) (size 0.6 0.25) (layers F.Cu))
  (pad 18 smd roundrect (roundrect_rratio 0.2) (at 2.04 -1.375) (size 0.25 0.65) (layers F.Cu))
  (pad 19 smd roundrect (roundrect_rratio 0.2) (at 1.54 -1.4) (size 0.25 0.6) (layers F.Cu))
  (pad 20 smd roundrect (roundrect_rratio 0.2) (at -1.54 -1.4) (size 0.25 0.6) (layers F.Cu))
  (pad 21 smd roundrect (roundrect_rratio 0.2) (at -2.04 -1.375) (size 0.25 0.65) (layers F.Cu))
  (pad 9 smd custom (at 0.0 0.0) (size 0.25 1.2) (layers F.Cu) (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy -0.165 -1.175)
          (xy -0.165 1.175)
          (xy -0.125 1.175)
          (xy -0.125 1.65)
          (xy -0.125 1.653)
          (xy -0.125 1.655)
          (xy -0.124 1.658)
          (xy -0.124 1.66)
          (xy -0.123 1.663)
          (xy -0.123 1.665)
          (xy -0.122 1.668)
          (xy -0.121 1.67)
          (xy -0.12 1.673)
          (xy -0.118 1.675)
          (xy -0.117 1.677)
          (xy -0.115 1.679)
          (xy -0.114 1.681)
          (xy -0.112 1.683)
          (xy -0.11 1.685)
          (xy -0.108 1.687)
          (xy -0.106 1.689)
          (xy -0.104 1.69)
          (xy -0.102 1.692)
          (xy -0.1 1.693)
          (xy -0.098 1.695)
          (xy -0.095 1.696)
          (xy -0.093 1.697)
          (xy -0.09 1.698)
          (xy -0.088 1.698)
          (xy -0.085 1.699)
          (xy -0.083 1.699)
          (xy -0.08 1.7)
          (xy -0.078 1.7)
          (xy -0.075 1.7)
          (xy 0.075 1.7)
          (xy 0.078 1.7)
          (xy 0.08 1.7)
          (xy 0.083 1.699)
          (xy 0.085 1.699)
          (xy 0.088 1.698)
          (xy 0.09 1.698)
          (xy 0.093 1.697)
          (xy 0.095 1.696)
          (xy 0.098 1.695)
          (xy 0.1 1.693)
          (xy 0.102 1.692)
          (xy 0.104 1.69)
          (xy 0.106 1.689)
          (xy 0.108 1.687)
          (xy 0.11 1.685)
          (xy 0.112 1.683)
          (xy 0.114 1.681)
          (xy 0.115 1.679)
          (xy 0.117 1.677)
          (xy 0.118 1.675)
          (xy 0.12 1.673)
          (xy 0.121 1.67)
          (xy 0.122 1.668)
          (xy 0.123 1.665)
          (xy 0.123 1.663)
          (xy 0.124 1.66)
          (xy 0.124 1.658)
          (xy 0.125 1.655)
          (xy 0.125 1.653)
          (xy 0.125 1.65)
          (xy 0.125 1.175)
          (xy 0.165 1.175)
          (xy 0.165 -1.175)
          (xy 0.125 -1.175)
          (xy 0.125 -1.65)
          (xy 0.125 -1.653)
          (xy 0.125 -1.655)
          (xy 0.124 -1.658)
          (xy 0.124 -1.66)
          (xy 0.123 -1.663)
          (xy 0.123 -1.665)
          (xy 0.122 -1.668)
          (xy 0.121 -1.67)
          (xy 0.12 -1.673)
          (xy 0.118 -1.675)
          (xy 0.117 -1.677)
          (xy 0.115 -1.679)
          (xy 0.114 -1.681)
          (xy 0.112 -1.683)
          (xy 0.11 -1.685)
          (xy 0.108 -1.687)
          (xy 0.106 -1.689)
          (xy 0.104 -1.69)
          (xy 0.102 -1.692)
          (xy 0.1 -1.693)
          (xy 0.098 -1.695)
          (xy 0.095 -1.696)
          (xy 0.093 -1.697)
          (xy 0.09 -1.698)
          (xy 0.088 -1.698)
          (xy 0.085 -1.699)
          (xy 0.083 -1.699)
          (xy 0.08 -1.7)
          (xy 0.078 -1.7)
          (xy 0.075 -1.7)
          (xy -0.075 -1.7)
          (xy -0.078 -1.7)
          (xy -0.08 -1.7)
          (xy -0.083 -1.699)
          (xy -0.085 -1.699)
          (xy -0.088 -1.698)
          (xy -0.09 -1.698)
          (xy -0.093 -1.697)
          (xy -0.095 -1.696)
          (xy -0.098 -1.695)
          (xy -0.1 -1.693)
          (xy -0.102 -1.692)
          (xy -0.104 -1.69)
          (xy -0.106 -1.689)
          (xy -0.108 -1.687)
          (xy -0.11 -1.685)
          (xy -0.112 -1.683)
          (xy -0.114 -1.681)
          (xy -0.115 -1.679)
          (xy -0.117 -1.677)
          (xy -0.118 -1.675)
          (xy -0.12 -1.673)
          (xy -0.121 -1.67)
          (xy -0.122 -1.668)
          (xy -0.123 -1.665)
          (xy -0.123 -1.663)
          (xy -0.124 -1.66)
          (xy -0.124 -1.658)
          (xy -0.125 -1.655)
          (xy -0.125 -1.653)
          (xy -0.125 -1.65)
          (xy -0.125 -1.175)
          (xy -0.165 -1.175)
        ) (width 0.01)
      )
    )
  )
)