(footprint "CR2032_HSN" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "CR2032_HSN" (at 0 1 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole circle (at -7.6 0) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 7.6 0) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask))
)
