(footprint "ChargR_ltc4162_v2" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "ChargR_ltc4162_v2" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 3.3 -18.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 3.3 -15.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at 0.76 -18.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "4" thru_hole oval (at 0.76 -15.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "5" thru_hole oval (at -1.78 -18.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "6" thru_hole oval (at -1.78 -15.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "7" thru_hole oval (at -4.32 -18.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "8" thru_hole oval (at -4.32 -15.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "9" thru_hole oval (at -6.86 -18.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "10" thru_hole oval (at -6.86 -15.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "11" thru_hole oval (at -9.4 -18.05 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "12" thru_hole oval (at -9.4 -15.51 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at -9.4 18.15 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "14" thru_hole oval (at -6.86 18.15 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "15" thru_hole oval (at -4.32 18.15 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "16" thru_hole oval (at -1.78 18.15 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "17" thru_hole oval (at 0.76 18.15 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "18" thru_hole rect (at 3.3 18.15 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "19" thru_hole circle (at 9.55 -16.85) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask))
  (pad "19" connect circle (at 9.55 -16.85) (size 5.6 5.6) (layers "F.Cu" "F.Mask"))
  (pad "19" connect circle (at 9.55 -16.85) (size 5.6 5.6) (layers "B.Cu" "B.Mask"))
  (pad "20" thru_hole circle (at 9.55 16.85) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask))
  (pad "20" connect circle (at 9.55 16.85) (size 5.6 5.6) (layers "B.Cu" "B.Mask"))
  (pad "20" connect circle (at 9.55 16.85) (size 5.6 5.6) (layers "F.Cu" "F.Mask"))
)
