(footprint "Coilcraft_XAL1350" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -7.62 unlocked) (layer "F.SilkS"))
  (fp_text value "Coilcraft_XAL1350" (at 0 -8.89 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 -1.27 unlocked) (layer "F.Fab"))
  (pad "1" smd roundrect (at -4.318 0 180) (size 2.9718 11.9888) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 4.318 0 180) (size 2.9718 11.9888) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
)
