(footprint "Coilcraft_XAL1580" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "Coilcraft_XAL1580" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at -0.1524 -0.635 unlocked) (layer "F.Fab"))
  (pad "1" smd roundrect (at -5.3086 0 180) (size 3.175 13.208) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 5.3086 0 180) (size 3.175 13.208) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
)
