(footprint "Cree_XHP70.3" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 1.58 -4.4 unlocked) (layer "F.SilkS"))
  (fp_text value "Cree_XHP70.3" (at 0.06 0 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 1.58 -4.4 unlocked) (layer "F.Fab"))
  (pad "1" smd roundrect (at -3.04 -2.04 90) (size 3.15 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -3.048 1.62 90) (size 3.15 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "3" smd roundrect (at 3.04 1.62 90) (size 3.15 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "4" smd roundrect (at 3.048 -2.04 90) (size 3.15 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "5" smd rect (at 0.01 -0.2 90) (size 6.8 4) (layers "F.Cu" "F.Paste" "F.Mask"))
)
