(footprint "DL-CC2340-A-40pin"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "DL-CC2340-A-40pin"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_rect
		(start 0 -26.5)
		(end 18 0)
		(fill none)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 0 -18.51)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at 0 -17.24)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 0 -15.97)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 0 -14.7)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 0 -13.43)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 0 -12.16)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 0 -10.89)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 0 -9.62)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 0 -8.35)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 0 -7.08)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 0 -5.81)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 0 -4.54)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 0 -3.27)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 0 -2)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at 2 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at 3.27 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at 4.54 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at 5.81 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd roundrect
		(at 7.08 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd roundrect
		(at 8.35 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "21" smd roundrect
		(at 9.62 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "22" smd roundrect
		(at 10.89 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "23" smd roundrect
		(at 12.16 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "24" smd roundrect
		(at 13.43 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "25" smd roundrect
		(at 14.7 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "26" smd roundrect
		(at 15.97 0 90)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "27" smd roundrect
		(at 18 -1.905)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "28" smd roundrect
		(at 18 -3.175)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "29" smd roundrect
		(at 18 -4.445)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "30" smd roundrect
		(at 18 -5.715)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "31" smd roundrect
		(at 18 -6.985)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "32" smd roundrect
		(at 18 -8.255)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "33" smd roundrect
		(at 18 -9.525)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "34" smd roundrect
		(at 18 -10.795)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "35" smd roundrect
		(at 18 -12.065)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "36" smd roundrect
		(at 18 -13.335)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "37" smd roundrect
		(at 18 -14.605)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "38" smd roundrect
		(at 18 -15.875)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "39" smd roundrect
		(at 18 -17.145)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "40" smd roundrect
		(at 18 -18.415)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
)
