(footprint "DL-CC2340-B-20pin"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.254 0.81 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "DL-CC2340-B-20pin"
		(at 0.254 2.31 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0.254 1.31 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0.254 1.31 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.254 1.31 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_rect
		(start 0 -18)
		(end 12 0)
		(fill none)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0.254 3.81 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 0 -12.192)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at 0 -10.922)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 0 -9.652)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 0 -8.382)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 0 -7.112)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 0 -5.842)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 0 -4.572)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 0 -3.302)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 0 -2.032)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 0 -0.762)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 12.065 -0.762)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 12.065 -2.032)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 12.065 -3.302)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 12.065 -4.572)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at 12.065 -5.842)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at 12.065 -7.112)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at 12.065 -8.382)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at 12.065 -9.652)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd roundrect
		(at 12.065 -10.922)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd roundrect
		(at 12.065 -12.192)
		(size 1.6 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
)
