(module CON10_2X5_DUK_FTSH_SAI (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CON10_2X5_DUK_FTSH_SAI (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 0) (layer F.SilkS))
  (fp_text user "*" (at 0 0) (layer F.Fab))
  (fp_text user "2" (at -3.683 -2.032) (layer F.SilkS))
  (fp_text user "2" (at -3.683 -2.032) (layer F.Fab))
  (fp_text user "1" (at -3.683 2.032) (layer F.SilkS))
  (fp_text user "1" (at -3.683 2.032) (layer F.Fab))
  (fp_text user "10" (at 3.683 -2.032) (layer F.SilkS))
  (fp_text user "10" (at 3.683 -2.032) (layer F.Fab))
  (fp_text user "9" (at 3.683 2.032) (layer F.SilkS))
  (fp_text user "9" (at 3.683 2.032) (layer F.Fab))
  (pad 1 smd rect (at -2.54 2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.54 -2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.27 2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.27 -2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0 -2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.27 2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.27 -2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 2.54 2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 2.54 -2.032) (size .762 2.794) (layers F.Cu F.Paste F.Mask))
)
