(footprint "HRS_DM3AT-SF-PEJM5" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6329ED27)
  (descr "Micro SD card holder with push-to-eject feature.")
  (attr through_hole)
  (fp_text reference "REF**" (at -3.98677 -2.43602) (layer "F.SilkS"))
  (fp_text value "HRS_DM3AT-SF-PEJM5" (at 5.55359 22.58781) (layer "F.Fab"))
  (fp_text user "PCB Edge" (at -4.75766 15.525) (layer "F.Fab"))
  (pad "1" smd rect (at 3.2 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 2.1 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 1 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -0.1 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -1.2 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -2.3 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -3.4 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -4.5 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "P1" smd rect (at -6.4 4.3) (size 1 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "P2" smd rect (at -6.4 14.65) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "P3" smd rect (at 7.1 15.1) (size 1.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "P4" smd rect (at 4.75 0) (size 1 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SWA" smd rect (at -6.4 10.5) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "SWB" smd rect (at -5.45 0) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.80394 4.9)
        (xy -6.05 4.9)
        (xy -6.05 8.50492)
        (xy -6.80394 8.50492)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.81306 0.45)
        (xy -6.05 0.45)
        (xy -6.05 3.70711)
        (xy -6.81306 3.70711)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -5.00324 5)
        (xy 3.7 5)
        (xy 3.7 6.60427)
        (xy -5.00324 6.60427)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -5.70605 6.3)
        (xy -5 6.3)
        (xy -5 13.9148)
        (xy -5.70605 13.9148)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 3.3515 14.7)
        (xy 5.9 14.7)
        (xy 5.9 16.0572)
        (xy 3.3515 16.0572)
      )
    )
  )
)
