(module LED_Cree-XD16_HandSoldering (layer F.Cu) (tedit 5E16AFD3)
  (descr "LED Cree-XQ handsoldering pads http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XQB.pdf")
  (tags "LED Cree XQ")
  (attr smd)
  (fp_text reference REF** (at 0 -2) (layer F.SilkS))
  (fp_text value LED_Cree-XD16_HandSoldering (at 0 2) (layer F.Fab))
  (fp_text user %R (at 0 0 180) (layer F.Fab))
  (pad 2 smd rect (at 0.88 0 180) (size 1.25 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.88 0 180) (size 1.25 1.6) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XQ.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
