(footprint "Launchpad-EK-TM4C123GXL"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -22.325 -34.135 0)
		(layer "F.SilkS")
	)
	(property "Value" "MODULE_EK-TM4C123GXL"
		(at -12.8 34.135 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "J1_1" thru_hole rect
		(at -22.86 -2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_2" thru_hole circle
		(at -22.86 0)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_3" thru_hole circle
		(at -22.86 2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_4" thru_hole circle
		(at -22.86 5.08)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_5" thru_hole circle
		(at -22.86 7.62)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_6" thru_hole circle
		(at -22.86 10.16)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_7" thru_hole circle
		(at -22.86 12.7)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_8" thru_hole circle
		(at -22.86 15.24)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_9" thru_hole circle
		(at -22.86 17.78)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J1_10" thru_hole circle
		(at -22.86 20.32)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_1" thru_hole circle
		(at 22.86 -2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_2" thru_hole circle
		(at 22.86 0)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_3" thru_hole circle
		(at 22.86 2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_4" thru_hole circle
		(at 22.86 5.08)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_5" thru_hole circle
		(at 22.86 7.62)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_6" thru_hole circle
		(at 22.86 10.16)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_7" thru_hole circle
		(at 22.86 12.7)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_8" thru_hole circle
		(at 22.86 15.24)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_9" thru_hole circle
		(at 22.86 17.78)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J2_10" thru_hole circle
		(at 22.86 20.32)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_1" thru_hole circle
		(at -20.32 -2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_2" thru_hole circle
		(at -20.32 0)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_3" thru_hole circle
		(at -20.32 2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_4" thru_hole circle
		(at -20.32 5.08)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_5" thru_hole circle
		(at -20.32 7.62)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_6" thru_hole circle
		(at -20.32 10.16)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_7" thru_hole circle
		(at -20.32 12.7)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_8" thru_hole circle
		(at -20.32 15.24)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_9" thru_hole circle
		(at -20.32 17.78)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J3_10" thru_hole circle
		(at -20.32 20.32)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_1" thru_hole circle
		(at 20.32 -2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_2" thru_hole circle
		(at 20.32 0)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_3" thru_hole circle
		(at 20.32 2.54)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_4" thru_hole circle
		(at 20.32 5.08)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_5" thru_hole circle
		(at 20.32 7.62)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_6" thru_hole circle
		(at 20.32 10.16)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_7" thru_hole circle
		(at 20.32 12.7)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_8" thru_hole circle
		(at 20.32 15.24)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_9" thru_hole circle
		(at 20.32 17.78)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "J4_10" thru_hole circle
		(at 20.32 20.32)
		(size 1.52 1.52)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
)
