(module M3-ATX-HV (layer F.Cu) (tedit 58D211DE)
  (fp_text reference REF** (at -8 5) (layer F.SilkS))
  (fp_text value M3-ATX-HV (at -6 -13.5) (layer F.Fab))
  (fp_text user 3V3 (at 11.8 19) (layer F.SilkS))
  (fp_text user -12V (at 11.8 14.8) (layer F.SilkS))
  (fp_text user GND (at 11.8 10.6) (layer F.SilkS))
  (fp_text user PS_ON (at 12.6 6.4) (layer F.SilkS))
  (fp_text user GND (at 11.8 2.2) (layer F.SilkS))
  (fp_text user GND (at 11.8 -2) (layer F.SilkS))
  (fp_text user GND (at 11.8 -6.2) (layer F.SilkS))
  (fp_text user 5V (at 11.4 -10.4) (layer F.SilkS))
  (fp_text user 5V (at 11.4 -14.6) (layer F.SilkS))
  (fp_text user GND (at 11.4 -18.8) (layer F.SilkS))
  (fp_text user 12V (at -1.4 -18.6) (layer F.SilkS))
  (fp_text user 5V_SB (at -2.2 -14.6) (layer F.SilkS))
  (fp_text user PWR_OK (at -2.8 -10.4) (layer F.SilkS))
  (fp_text user GND (at -1.6 -6.2) (layer F.SilkS))
  (fp_text user 5V (at -1.6 -2) (layer F.SilkS))
  (fp_text user GND (at -1.6 2.2) (layer F.SilkS))
  (fp_text user 5V (at -1.6 6.4) (layer F.SilkS))
  (fp_text user GND (at -1.6 10.6) (layer F.SilkS))
  (fp_text user 3V3 (at -1.6 15) (layer F.SilkS))
  (fp_text user 3V3 (at -1.6 19.2) (layer F.SilkS))
  (pad 1 thru_hole circle (at 2.2 19.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.2 14.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.2 10.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.2 6.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 2.2 2.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.2 -1.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 2.2 -6.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 2.2 -10.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 2.2 -14.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 2.2 -18.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 7.7 19.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 7.7 14.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 7.7 10.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 7.7 6.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 7.7 2.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 7.7 -1.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 7.7 -6.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 7.7 -10.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 7.7 -14.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 7.7 -18.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask))
)
