(footprint "ML2020_F1AN" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62DC3AF7)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 0) (layer "F.SilkS"))
  (fp_text value "ML2020/F1AN" (at 0 0) (layer "F.Fab"))
  (pad "1" smd rect (at -10.8 7.55 35) (size 2 3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 13 0) (size 2 3) (layers "F.Cu" "F.Paste" "F.Mask"))
)
