(footprint "PCA6408A_SOP65P640X110-16N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.762 -4.064 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOP65P640X110-16N"
		(at 0.254 5.08 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -2.8702 -2.286)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "2" smd rect
		(at -2.8702 -1.6256)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "3" smd rect
		(at -2.8702 -0.9652)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "4" smd rect
		(at -2.8702 -0.3302)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "5" smd rect
		(at -2.8702 0.3302)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "6" smd rect
		(at -2.8702 0.9652)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "7" smd rect
		(at -2.8702 1.6256)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "8" smd rect
		(at -2.8702 2.286)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "9" smd rect
		(at 2.8702 2.286)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "10" smd rect
		(at 2.8702 1.6256)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "11" smd rect
		(at 2.8702 0.9652)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "12" smd rect
		(at 2.8702 0.3302)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "13" smd rect
		(at 2.8702 -0.3302)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "14" smd rect
		(at 2.8702 -0.9652)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "15" smd rect
		(at 2.8702 -1.6256)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
	(pad "16" smd rect
		(at 2.8702 -2.286)
		(size 1.4732 0.3556)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.102)
	)
)
