(footprint "Pulse_PM5433" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "Pulse_PM5433" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at -0.1524 -1.143 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 1.992 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -5.3086 0 180) (size 4.5 15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 5.3086 0 180) (size 4.5 15) (layers "F.Cu" "F.Paste" "F.Mask"))
)
